(kicad_pcb (version 20171130) (host pcbnew 5.1.4+dfsg1-1)
  (general
    (thickness 1.6)
    (drawings 109)
    (tracks 64)
    (zones 0)
    (modules 5)
    (nets 5)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 Board_1-/BP_B1+)
  (net 2 Board_1-/BP_B1-)
  (net 3 Board_1-/BP_B2+)
  (net 4 Board_1-/BP_B2-)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net Board_1-/BP_B1+)
    (add_net Board_1-/BP_B1-)
    (add_net Board_1-/BP_B2+)
    (add_net Board_1-/BP_B2-)
  )
  (module batteryPack:2mm_Banana-Socket (layer F.Cu) (tedit 5E838ADF)
    (at 165 111 270)
    (fp_text reference J9 (at 0 16.5 90) (layer F.SilkS) hide)
    (fp_text value B2+ (at 0 -1.25 90) (layer F.Fab))
    (pad 1 smd rect (at 0 7.5 270) (size 3 15) (layers F.Cu F.Paste F.Mask)
      (net 3 Board_1-/BP_B2+))
  )
  (module batteryPack:2mm_Banana-Socket (layer F.Cu) (tedit 5E838ADF)
    (at 165 91 270)
    (fp_text reference J10 (at 0 16.5 90) (layer F.SilkS) hide)
    (fp_text value B1+ (at 0 -1.25 90) (layer F.Fab))
    (pad 1 smd rect (at 0 7.5 270) (size 3 15) (layers F.Cu F.Paste F.Mask)
      (net 1 Board_1-/BP_B1+))
  )
  (module batteryPack:2mm_Banana-Socket (layer F.Cu) (tedit 5E838ADF)
    (at 165 98 270)
    (fp_text reference J11 (at 0 16.5 90) (layer F.SilkS) hide)
    (fp_text value B1- (at 0 -1.25 90) (layer F.Fab))
    (pad 1 smd rect (at 0 7.5 270) (size 3 15) (layers F.Cu F.Paste F.Mask)
      (net 2 Board_1-/BP_B1-))
  )
  (module batteryPack:2mm_Banana-Socket (layer F.Cu) (tedit 5E838ADF)
    (at 165 104 270)
    (fp_text reference J12 (at 0 16.5 90) (layer F.SilkS) hide)
    (fp_text value B2- (at 0 -1.25 90) (layer F.Fab))
    (pad 1 smd rect (at 0 7.5 270) (size 3 15) (layers F.Cu F.Paste F.Mask)
      (net 4 Board_1-/BP_B2-))
  )
  (module batteryPack:BAT_BK-18650-PC4 (layer B.Cu) (tedit 5EEA42C1)
    (at 145 101 270)
    (fp_text reference BT1 (at -36.195 19.05 90) (layer B.SilkS) hide)
    (fp_text value BK-18650-PC4 (at -28.84 -19.05 90) (layer B.Fab))
    (pad 1+ thru_hole oval (at -36.2 9.6 270) (size 3 4) (drill oval 1 2) (layers *.Cu *.Mask)
      (net 1 Board_1-/BP_B1+))
    (pad 1 thru_hole oval (at 36.2 9.6 270) (size 3 4) (drill oval 1 2) (layers *.Cu *.Mask)
      (net 2 Board_1-/BP_B1-))
    (pad 2 thru_hole oval (at 36.2 -9.6 270) (size 3 4) (drill oval 1 2) (layers *.Cu *.Mask)
      (net 4 Board_1-/BP_B2-))
    (pad 2+ thru_hole oval (at -36.2 -9.6 270) (size 3 4) (drill oval 1 2) (layers *.Cu *.Mask)
      (net 3 Board_1-/BP_B2+))
    (model C:/Users/mp363/Desktop/BK-18650-PC4/BAT_BK-18650-PC4.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -90))
    )
  )
  (gr_line (start 164.1046 139.9955) (end 164 140.001) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164.2081 139.9791) (end 164.1046 139.9955) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164.3093 139.952) (end 164.2081 139.9791) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164.4071 139.9145) (end 164.3093 139.952) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164.5005 139.8669) (end 164.4071 139.9145) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164.5883 139.8099) (end 164.5005 139.8669) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164.6698 139.7439) (end 164.5883 139.8099) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164.7439 139.6698) (end 164.6698 139.7439) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164.8099 139.5883) (end 164.7439 139.6698) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164.8669 139.5005) (end 164.8099 139.5883) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164.9145 139.4071) (end 164.8669 139.5005) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164.952 139.3093) (end 164.9145 139.4071) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164.9791 139.2081) (end 164.952 139.3093) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164.9955 139.1046) (end 164.9791 139.2081) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 165.001 139) (end 164.9955 139.1046) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 165.001 63) (end 165.001 139) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164.9955 62.8953) (end 165.001 63) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164.9791 62.7918) (end 164.9955 62.8953) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164.952 62.6906) (end 164.9791 62.7918) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164.9144 62.5928) (end 164.952 62.6906) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164.8669 62.4995) (end 164.9144 62.5928) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164.8099 62.4117) (end 164.8669 62.4995) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164.7439 62.3302) (end 164.8099 62.4117) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164.6698 62.2561) (end 164.7439 62.3302) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164.5884 62.1902) (end 164.6698 62.2561) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164.5005 62.1331) (end 164.5884 62.1902) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164.4071 62.0855) (end 164.5005 62.1331) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164.3093 62.048) (end 164.4071 62.0855) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164.2081 62.0209) (end 164.3093 62.048) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164.1047 62.0045) (end 164.2081 62.0209) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164 61.999) (end 164.1047 62.0045) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 126 61.999) (end 164 61.999) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 125.8953 62.0045) (end 126 61.999) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 125.7918 62.0209) (end 125.8953 62.0045) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 125.6906 62.048) (end 125.7918 62.0209) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 125.5928 62.0856) (end 125.6906 62.048) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 125.4995 62.1331) (end 125.5928 62.0856) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 125.4117 62.1901) (end 125.4995 62.1331) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 125.3302 62.2561) (end 125.4117 62.1901) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 125.2561 62.3302) (end 125.3302 62.2561) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 125.1902 62.4116) (end 125.2561 62.3302) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 125.1331 62.4995) (end 125.1902 62.4116) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 125.0856 62.5928) (end 125.1331 62.4995) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 125.048 62.6907) (end 125.0856 62.5928) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 125.0209 62.7918) (end 125.048 62.6907) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 125.0045 62.8953) (end 125.0209 62.7918) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 124.999 63) (end 125.0045 62.8953) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 124.999 139) (end 124.999 63) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 125.0045 139.1047) (end 124.999 139) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 125.0209 139.2082) (end 125.0045 139.1047) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 125.048 139.3094) (end 125.0209 139.2082) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 125.0856 139.4072) (end 125.048 139.3094) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 125.1331 139.5005) (end 125.0856 139.4072) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 125.1901 139.5883) (end 125.1331 139.5005) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 125.2561 139.6698) (end 125.1901 139.5883) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 125.3302 139.7439) (end 125.2561 139.6698) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 125.4117 139.8099) (end 125.3302 139.7439) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 125.4995 139.8669) (end 125.4117 139.8099) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 125.5929 139.9145) (end 125.4995 139.8669) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 125.6907 139.952) (end 125.5929 139.9145) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 125.7919 139.9791) (end 125.6907 139.952) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 125.8953 139.9955) (end 125.7919 139.9791) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 126 140.001) (end 125.8953 139.9955) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164 140.001) (end 126 140.001) (layer Edge.Cuts) (width 0.1))
  (gr_text + (at 148 91 90) (layer F.SilkS))
  (gr_text _ (at 146.75 98.25 90) (layer F.SilkS))
  (gr_text _ (at 146.75 103.75 90) (layer F.SilkS))
  (gr_text + (at 148.25 111 90) (layer F.SilkS))
  (gr_text B2 (at 148.25 107.5 90) (layer F.SilkS))
  (gr_text B1 (at 148 94.75 90) (layer F.SilkS))
  (gr_text B1+ (at 135.75 68.25) (layer F.SilkS))
  (gr_text B2+ (at 155.25 68.25) (layer F.SilkS))
  (gr_text B2- (at 155 134.25) (layer F.SilkS))
  (gr_text B1- (at 136 134.25) (layer F.SilkS))
  (gr_text "RB0002 Battery Pack\nBattery Board\nv1.0     06/2020     CC BY-SA 4.0\ngithub.com/RoboticsBrno/RB0002-BatteryPack" (at 141 100 90) (layer F.SilkS))
  (gr_text "Panel tab position" (at 175.5 68) (layer Cmts.User))
  (gr_text "Panel tab position" (at 175.5 84.5) (layer Cmts.User))
  (gr_text "Panel tab position" (at 175.25 117.75) (layer Cmts.User))
  (gr_text "Panel tab position" (at 175.5 134) (layer Cmts.User))
  (zone (net 1) (net_name Board_1-/BP_B1+) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 1))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 1) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 165 93) (xy 125.9 93.375) (xy 125.9 62.375) (xy 165 62)
      )
    )
  )
  (zone (net 2) (net_name Board_1-/BP_B1-) (layer F.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 1))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 1) (smoothing fillet))
    (polygon
      (pts
        (xy 125.275 93.1) (xy 165 93) (xy 165 140) (xy 125.275 140.1)
      )
    )
  )
  (zone (net 4) (net_name Board_1-/BP_B2-) (layer F.Cu) (hatch edge 0.508)
    (priority 3)
    (connect_pads yes (clearance 1))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 1) (smoothing fillet))
    (polygon
      (pts
        (xy 165 140) (xy 165 102) (xy 139.625 102.05) (xy 139.625 140.05)
      )
    )
  )
  (zone (net 3) (net_name Board_1-/BP_B2+) (layer B.Cu) (hatch edge 0.508)
    (priority 3)
    (connect_pads yes (clearance 1))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 1) (smoothing fillet) (radius 2))
    (polygon
      (pts
        (xy 132 62) (xy 132 114) (xy 165 114) (xy 165 108) (xy 149.5 108)
        (xy 149.5 90) (xy 165 90) (xy 165 62)
      )
    )
  )
)
