(kicad_pcb (version 20171130) (host pcbnew 5.1.5+dfsg1-2build2)
  (general
    (thickness 1.6)
    (drawings 760)
    (tracks 1212)
    (zones 0)
    (modules 252)
    (nets 121)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 0 0)
    (grid_origin 132.08 72.39)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 Board_1-+3V3)
  (net 2 Board_1-+5V)
  (net 3 Board_1-BUTTON)
  (net 4 Board_1-D+)
  (net 5 Board_1-D-)
  (net 6 Board_1-DTR)
  (net 7 Board_1-GND)
  (net 8 Board_1-LED-A)
  (net 9 Board_1-LED-B)
  (net 10 Board_1-LED-C)
  (net 11 "Board_1-Net-(C3-Pad1)")
  (net 12 "Board_1-Net-(C5-Pad1)")
  (net 13 "Board_1-Net-(D1-Pad1)")
  (net 14 "Board_1-Net-(D3-Pad1)")
  (net 15 "Board_1-Net-(D5-Pad1)")
  (net 16 "Board_1-Net-(Q1-Pad1)")
  (net 17 "Board_1-Net-(Q1-Pad3)")
  (net 18 "Board_1-Net-(Q2-Pad1)")
  (net 19 "Board_1-Net-(Q2-Pad3)")
  (net 20 "Board_1-Net-(Q3-Pad1)")
  (net 21 "Board_1-Net-(Q3-Pad3)")
  (net 22 "Board_1-Net-(R8-Pad2)")
  (net 23 "Board_1-Net-(R9-Pad2)")
  (net 24 "Board_1-Net-(U3-Pad10)")
  (net 25 "Board_1-Net-(U3-Pad11)")
  (net 26 "Board_1-Net-(U3-Pad12)")
  (net 27 "Board_1-Net-(U3-Pad15)")
  (net 28 "Board_1-Net-(U3-Pad9)")
  (net 29 Board_1-RESET)
  (net 30 Board_1-RTS)
  (net 31 Board_2-+3V3)
  (net 32 Board_2-+5V)
  (net 33 Board_2-BUTTON)
  (net 34 Board_2-D+)
  (net 35 Board_2-D-)
  (net 36 Board_2-DTR)
  (net 37 Board_2-GND)
  (net 38 Board_2-LED-A)
  (net 39 Board_2-LED-B)
  (net 40 Board_2-LED-C)
  (net 41 "Board_2-Net-(C3-Pad1)")
  (net 42 "Board_2-Net-(C5-Pad1)")
  (net 43 "Board_2-Net-(D1-Pad1)")
  (net 44 "Board_2-Net-(D3-Pad1)")
  (net 45 "Board_2-Net-(D5-Pad1)")
  (net 46 "Board_2-Net-(Q1-Pad1)")
  (net 47 "Board_2-Net-(Q1-Pad3)")
  (net 48 "Board_2-Net-(Q2-Pad1)")
  (net 49 "Board_2-Net-(Q2-Pad3)")
  (net 50 "Board_2-Net-(Q3-Pad1)")
  (net 51 "Board_2-Net-(Q3-Pad3)")
  (net 52 "Board_2-Net-(R8-Pad2)")
  (net 53 "Board_2-Net-(R9-Pad2)")
  (net 54 "Board_2-Net-(U3-Pad10)")
  (net 55 "Board_2-Net-(U3-Pad11)")
  (net 56 "Board_2-Net-(U3-Pad12)")
  (net 57 "Board_2-Net-(U3-Pad15)")
  (net 58 "Board_2-Net-(U3-Pad9)")
  (net 59 Board_2-RESET)
  (net 60 Board_2-RTS)
  (net 61 Board_3-+3V3)
  (net 62 Board_3-+5V)
  (net 63 Board_3-BUTTON)
  (net 64 Board_3-D+)
  (net 65 Board_3-D-)
  (net 66 Board_3-DTR)
  (net 67 Board_3-GND)
  (net 68 Board_3-LED-A)
  (net 69 Board_3-LED-B)
  (net 70 Board_3-LED-C)
  (net 71 "Board_3-Net-(C3-Pad1)")
  (net 72 "Board_3-Net-(C5-Pad1)")
  (net 73 "Board_3-Net-(D1-Pad1)")
  (net 74 "Board_3-Net-(D3-Pad1)")
  (net 75 "Board_3-Net-(D5-Pad1)")
  (net 76 "Board_3-Net-(Q1-Pad1)")
  (net 77 "Board_3-Net-(Q1-Pad3)")
  (net 78 "Board_3-Net-(Q2-Pad1)")
  (net 79 "Board_3-Net-(Q2-Pad3)")
  (net 80 "Board_3-Net-(Q3-Pad1)")
  (net 81 "Board_3-Net-(Q3-Pad3)")
  (net 82 "Board_3-Net-(R8-Pad2)")
  (net 83 "Board_3-Net-(R9-Pad2)")
  (net 84 "Board_3-Net-(U3-Pad10)")
  (net 85 "Board_3-Net-(U3-Pad11)")
  (net 86 "Board_3-Net-(U3-Pad12)")
  (net 87 "Board_3-Net-(U3-Pad15)")
  (net 88 "Board_3-Net-(U3-Pad9)")
  (net 89 Board_3-RESET)
  (net 90 Board_3-RTS)
  (net 91 Board_4-+3V3)
  (net 92 Board_4-+5V)
  (net 93 Board_4-BUTTON)
  (net 94 Board_4-D+)
  (net 95 Board_4-D-)
  (net 96 Board_4-DTR)
  (net 97 Board_4-GND)
  (net 98 Board_4-LED-A)
  (net 99 Board_4-LED-B)
  (net 100 Board_4-LED-C)
  (net 101 "Board_4-Net-(C3-Pad1)")
  (net 102 "Board_4-Net-(C5-Pad1)")
  (net 103 "Board_4-Net-(D1-Pad1)")
  (net 104 "Board_4-Net-(D3-Pad1)")
  (net 105 "Board_4-Net-(D5-Pad1)")
  (net 106 "Board_4-Net-(Q1-Pad1)")
  (net 107 "Board_4-Net-(Q1-Pad3)")
  (net 108 "Board_4-Net-(Q2-Pad1)")
  (net 109 "Board_4-Net-(Q2-Pad3)")
  (net 110 "Board_4-Net-(Q3-Pad1)")
  (net 111 "Board_4-Net-(Q3-Pad3)")
  (net 112 "Board_4-Net-(R8-Pad2)")
  (net 113 "Board_4-Net-(R9-Pad2)")
  (net 114 "Board_4-Net-(U3-Pad10)")
  (net 115 "Board_4-Net-(U3-Pad11)")
  (net 116 "Board_4-Net-(U3-Pad12)")
  (net 117 "Board_4-Net-(U3-Pad15)")
  (net 118 "Board_4-Net-(U3-Pad9)")
  (net 119 Board_4-RESET)
  (net 120 Board_4-RTS)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net Board_1-+3V3)
    (add_net Board_1-+5V)
    (add_net Board_1-BUTTON)
    (add_net Board_1-D+)
    (add_net Board_1-D-)
    (add_net Board_1-DTR)
    (add_net Board_1-GND)
    (add_net Board_1-LED-A)
    (add_net Board_1-LED-B)
    (add_net Board_1-LED-C)
    (add_net "Board_1-Net-(C3-Pad1)")
    (add_net "Board_1-Net-(C5-Pad1)")
    (add_net "Board_1-Net-(D1-Pad1)")
    (add_net "Board_1-Net-(D3-Pad1)")
    (add_net "Board_1-Net-(D5-Pad1)")
    (add_net "Board_1-Net-(Q1-Pad1)")
    (add_net "Board_1-Net-(Q1-Pad3)")
    (add_net "Board_1-Net-(Q2-Pad1)")
    (add_net "Board_1-Net-(Q2-Pad3)")
    (add_net "Board_1-Net-(Q3-Pad1)")
    (add_net "Board_1-Net-(Q3-Pad3)")
    (add_net "Board_1-Net-(R8-Pad2)")
    (add_net "Board_1-Net-(R9-Pad2)")
    (add_net "Board_1-Net-(U3-Pad10)")
    (add_net "Board_1-Net-(U3-Pad11)")
    (add_net "Board_1-Net-(U3-Pad12)")
    (add_net "Board_1-Net-(U3-Pad15)")
    (add_net "Board_1-Net-(U3-Pad9)")
    (add_net Board_1-RESET)
    (add_net Board_1-RTS)
    (add_net Board_2-+3V3)
    (add_net Board_2-+5V)
    (add_net Board_2-BUTTON)
    (add_net Board_2-D+)
    (add_net Board_2-D-)
    (add_net Board_2-DTR)
    (add_net Board_2-GND)
    (add_net Board_2-LED-A)
    (add_net Board_2-LED-B)
    (add_net Board_2-LED-C)
    (add_net "Board_2-Net-(C3-Pad1)")
    (add_net "Board_2-Net-(C5-Pad1)")
    (add_net "Board_2-Net-(D1-Pad1)")
    (add_net "Board_2-Net-(D3-Pad1)")
    (add_net "Board_2-Net-(D5-Pad1)")
    (add_net "Board_2-Net-(Q1-Pad1)")
    (add_net "Board_2-Net-(Q1-Pad3)")
    (add_net "Board_2-Net-(Q2-Pad1)")
    (add_net "Board_2-Net-(Q2-Pad3)")
    (add_net "Board_2-Net-(Q3-Pad1)")
    (add_net "Board_2-Net-(Q3-Pad3)")
    (add_net "Board_2-Net-(R8-Pad2)")
    (add_net "Board_2-Net-(R9-Pad2)")
    (add_net "Board_2-Net-(U3-Pad10)")
    (add_net "Board_2-Net-(U3-Pad11)")
    (add_net "Board_2-Net-(U3-Pad12)")
    (add_net "Board_2-Net-(U3-Pad15)")
    (add_net "Board_2-Net-(U3-Pad9)")
    (add_net Board_2-RESET)
    (add_net Board_2-RTS)
    (add_net Board_3-+3V3)
    (add_net Board_3-+5V)
    (add_net Board_3-BUTTON)
    (add_net Board_3-D+)
    (add_net Board_3-D-)
    (add_net Board_3-DTR)
    (add_net Board_3-GND)
    (add_net Board_3-LED-A)
    (add_net Board_3-LED-B)
    (add_net Board_3-LED-C)
    (add_net "Board_3-Net-(C3-Pad1)")
    (add_net "Board_3-Net-(C5-Pad1)")
    (add_net "Board_3-Net-(D1-Pad1)")
    (add_net "Board_3-Net-(D3-Pad1)")
    (add_net "Board_3-Net-(D5-Pad1)")
    (add_net "Board_3-Net-(Q1-Pad1)")
    (add_net "Board_3-Net-(Q1-Pad3)")
    (add_net "Board_3-Net-(Q2-Pad1)")
    (add_net "Board_3-Net-(Q2-Pad3)")
    (add_net "Board_3-Net-(Q3-Pad1)")
    (add_net "Board_3-Net-(Q3-Pad3)")
    (add_net "Board_3-Net-(R8-Pad2)")
    (add_net "Board_3-Net-(R9-Pad2)")
    (add_net "Board_3-Net-(U3-Pad10)")
    (add_net "Board_3-Net-(U3-Pad11)")
    (add_net "Board_3-Net-(U3-Pad12)")
    (add_net "Board_3-Net-(U3-Pad15)")
    (add_net "Board_3-Net-(U3-Pad9)")
    (add_net Board_3-RESET)
    (add_net Board_3-RTS)
    (add_net Board_4-+3V3)
    (add_net Board_4-+5V)
    (add_net Board_4-BUTTON)
    (add_net Board_4-D+)
    (add_net Board_4-D-)
    (add_net Board_4-DTR)
    (add_net Board_4-GND)
    (add_net Board_4-LED-A)
    (add_net Board_4-LED-B)
    (add_net Board_4-LED-C)
    (add_net "Board_4-Net-(C3-Pad1)")
    (add_net "Board_4-Net-(C5-Pad1)")
    (add_net "Board_4-Net-(D1-Pad1)")
    (add_net "Board_4-Net-(D3-Pad1)")
    (add_net "Board_4-Net-(D5-Pad1)")
    (add_net "Board_4-Net-(Q1-Pad1)")
    (add_net "Board_4-Net-(Q1-Pad3)")
    (add_net "Board_4-Net-(Q2-Pad1)")
    (add_net "Board_4-Net-(Q2-Pad3)")
    (add_net "Board_4-Net-(Q3-Pad1)")
    (add_net "Board_4-Net-(Q3-Pad3)")
    (add_net "Board_4-Net-(R8-Pad2)")
    (add_net "Board_4-Net-(R9-Pad2)")
    (add_net "Board_4-Net-(U3-Pad10)")
    (add_net "Board_4-Net-(U3-Pad11)")
    (add_net "Board_4-Net-(U3-Pad12)")
    (add_net "Board_4-Net-(U3-Pad15)")
    (add_net "Board_4-Net-(U3-Pad9)")
    (add_net Board_4-RESET)
    (add_net Board_4-RTS)
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 91.253337 126.329022)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 90.253337 126.329021)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 89.253337 126.329021)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 88.253337 126.32902)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 87.253337 126.329019)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 86.253337 126.329019)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 85.253337 126.329018)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 84.253337 126.329017)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 83.253337 126.329017)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 72.626668 126.32901)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 71.626668 126.32901)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 70.626668 126.329009)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 69.626668 126.329008)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 68.626668 126.329008)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 67.626668 126.329007)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 66.626668 126.329006)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 65.626668 126.329006)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 64.626668 126.329005)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 83.253338 123.330966)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 84.253338 123.330968)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 85.253338 123.33097)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 86.253338 123.330972)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 87.253338 123.330974)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 88.253338 123.330976)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 89.253338 123.330978)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 90.253338 123.33098)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 91.253338 123.330982)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 64.626669 123.330928)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 65.626669 123.33093)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 66.626669 123.330932)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 67.626669 123.330934)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 68.626669 123.330936)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 69.626669 123.330938)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 70.626669 123.33094)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 71.626669 123.330942)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 72.626669 123.330944)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 91.253337 100.969015)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 90.253337 100.969014)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 89.253337 100.969014)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 88.253337 100.969013)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 87.253337 100.969013)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 86.253337 100.969013)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 85.253337 100.969012)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 84.253337 100.969012)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 83.253337 100.969011)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 72.626668 100.969007)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 71.626668 100.969006)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 70.626668 100.969006)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 69.626668 100.969005)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 68.626668 100.969005)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 67.626668 100.969005)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 66.626668 100.969004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 65.626668 100.969004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 64.626668 100.969003)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 83.253338 97.970962)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 84.253338 97.970964)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 85.253338 97.970967)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 86.253338 97.970969)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 87.253338 97.970971)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 88.253338 97.970973)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 89.253338 97.970975)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 90.253338 97.970978)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 91.253338 97.97098)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 64.626669 97.970921)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 65.626669 97.970923)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 66.626669 97.970926)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 67.626669 97.970928)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 68.626669 97.97093)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 69.626669 97.970932)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 70.626669 97.970934)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 71.626669 97.970937)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 72.626669 97.970939)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 91.253337 75.609007)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 90.253337 75.609007)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 89.253337 75.609007)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 88.253337 75.609007)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 87.253337 75.609007)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 86.253337 75.609006)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 85.253337 75.609006)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 84.253337 75.609006)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 83.253337 75.609006)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 72.626668 75.609003)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 71.626668 75.609003)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 70.626668 75.609003)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 69.626668 75.609003)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 68.626668 75.609002)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 67.626668 75.609002)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 66.626668 75.609002)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 65.626668 75.609002)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 64.626668 75.609002)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 83.253338 72.610959)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 84.253338 72.610961)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 85.253338 72.610964)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 86.253338 72.610966)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 87.253338 72.610968)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 88.253338 72.610971)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 89.253338 72.610973)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 90.253338 72.610976)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 91.253338 72.610978)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 64.626669 72.610914)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 65.626669 72.610916)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 66.626669 72.610919)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 67.626669 72.610921)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 68.626669 72.610924)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 69.626669 72.610926)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 70.626669 72.610928)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 71.626669 72.610931)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 72.626669 72.610933)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module Capacitor_THT:CP_Radial_D6.3mm_P2.50mm (layer B.Cu) (tedit 5AE50EF0)
    (at 62.700001 132.430028)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (fp_text reference C1 (at -2.54 -1.905 180) (layer B.SilkS))
    (fp_text value 47uF (at 1.25 -4.4 180) (layer B.Fab))
    (fp_text user %R (at 1.25 0 180) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 91 Board_4-+3V3))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 97 Board_4-GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 97.625001 139.197528 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0.8525 -1.905 90) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.82 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 106 "Board_4-Net-(Q1-Pad1)"))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 98 Board_4-LED-A))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 101.435001 139.197528 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at 0 -1.905 90) (layer B.SilkS))
    (fp_text value 33k (at 0 -1.82 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 108 "Board_4-Net-(Q2-Pad1)"))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 99 Board_4-LED-B))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 93.815001 139.197528 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at -0.8525 1.905 90) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.82 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 110 "Board_4-Net-(Q3-Pad1)"))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 100 Board_4-LED-C))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 60.160001 144.913028 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at 0 1.82 90) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.82 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 93 Board_4-BUTTON))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 91 Board_4-+3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 95.720001 129.672528 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R5 (at 0 1.82 90) (layer B.Fab))
    (fp_text value 75R (at 0 -1.82 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 103 "Board_4-Net-(D1-Pad1)"))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 107 "Board_4-Net-(Q1-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 83.437001 129.255028)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R6 (at 0 1.82) (layer B.Fab))
    (fp_text value 75R (at 0 -1.82) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 109 "Board_4-Net-(Q2-Pad3)"))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 104 "Board_4-Net-(D3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 99.947001 129.255028 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R7 (at 0 1.82) (layer B.SilkS))
    (fp_text value 75R (at 0 -1.82) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0 180) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 105 "Board_4-Net-(D5-Pad1)"))
    (pad 2 smd roundrect (at 1.4875 0 180) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 111 "Board_4-Net-(Q3-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 86.195001 139.197528 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R8 (at -0.8525 1.905 90) (layer B.SilkS))
    (fp_text value 1k (at 0 -1.82 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 98 Board_4-LED-A))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 112 "Board_4-Net-(R8-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 90.005001 139.197528 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R9 (at 0.8525 -1.905 90) (layer B.Fab))
    (fp_text value 1k (at 0 -1.82 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 100 Board_4-LED-C))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 113 "Board_4-Net-(R9-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_THT:SW_PUSH_6mm (layer F.Cu) (tedit 5A02FE31)
    (at 69.685001 147.035028 180)
    (descr https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "tact sw push 6mm")
    (fp_text reference SW1 (at 9.398 -0.635) (layer F.Fab))
    (fp_text value SW_Push (at 3.75 6.7) (layer F.Fab))
    (fp_text user %R (at 3.25 2.25) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 4.5 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 97 Board_4-GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 93 Board_4-BUTTON))
    (pad 2 thru_hole circle (at 6.5 4.5 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 97 Board_4-GND))
    (pad 1 thru_hole circle (at 6.5 0 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 93 Board_4-BUTTON))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_PUSH_6mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-223-3_TabPin2 (layer B.Cu) (tedit 5A02FF57)
    (at 55.690001 137.510028 180)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U2 (at 3.277 2.921) (layer B.SilkS))
    (fp_text value AMS1117-3.3 (at 0 -4.5) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd rect (at 3.15 0 180) (size 2 3.8) (layers B.Cu B.Paste B.Mask)
      (net 91 Board_4-+3V3))
    (pad 2 smd rect (at -3.15 0 180) (size 2 1.5) (layers B.Cu B.Paste B.Mask)
      (net 91 Board_4-+3V3))
    (pad 3 smd rect (at -3.15 -2.3 180) (size 2 1.5) (layers B.Cu B.Paste B.Mask)
      (net 92 Board_4-+5V))
    (pad 1 smd rect (at -3.15 2.3 180) (size 2 1.5) (layers B.Cu B.Paste B.Mask)
      (net 97 Board_4-GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module semaforBoard:ESP-01 (layer B.Cu) (tedit 5EC82F3F)
    (at 91.275001 136.240028 90)
    (fp_text reference U1 (at -8.89 4.445 90) (layer B.Fab))
    (fp_text value ESP-01 (at -12.065 -1.27 180) (layer B.SilkS))
    (pad 1 thru_hole circle (at -10.16 -5.08 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 91 Board_4-+3V3))
    (pad 2 thru_hole circle (at -7.62 2.54 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 97 Board_4-GND))
    (pad 3 thru_hole circle (at -10.16 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 91 Board_4-+3V3))
    (pad 4 thru_hole circle (at -10.16 -2.54 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 119 Board_4-RESET))
    (pad 5 thru_hole circle (at -7.62 -2.54 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 93 Board_4-BUTTON))
    (pad 6 thru_hole circle (at -10.16 2.54 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 98 Board_4-LED-A))
    (pad 7 thru_hole circle (at -7.62 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 99 Board_4-LED-B))
    (pad 8 thru_hole circle (at -7.62 -5.08 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 100 Board_4-LED-C))
    (model "D:/Robotarna/Semafor/hw/ESP-01-fixed v3.step"
      (offset (xyz 0.8 -1.2 3))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module semaforBoard:USB_A_CNCTech_1001-011-01101_Horizontal (layer F.Cu) (tedit 5EC84A2B)
    (at 77.925001 152.665028 270)
    (descr "USB type A Plug, Horizontal, http://cnctech.us/pdfs/1001-011-01101.pdf")
    (tags USB-A)
    (attr smd)
    (fp_text reference J3 (at -6.9 -8 90) (layer F.Fab))
    (fp_text value USB_A (at -4.995 -0.015) (layer F.Fab))
    (fp_text user "PCB Edge" (at -4.55 -0.05) (layer Dwgs.User))
    (fp_text user %R (at -6 0) (layer F.Fab))
    (pad 2 smd rect (at -9.65 -1 270) (size 2.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 95 Board_4-D-))
    (pad 3 smd rect (at -9.65 1 270) (size 2.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 94 Board_4-D+))
    (pad 1 smd rect (at -9.65 -3.5 270) (size 2.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 92 Board_4-+5V))
    (pad 4 smd rect (at -9.65 3.5 270) (size 2.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 97 Board_4-GND))
    (pad 5 thru_hole oval (at -6.9 -5.7 270) (size 3.5 1.9) (drill oval 2.5 0.9) (layers *.Cu *.Mask)
      (net 97 Board_4-GND))
    (pad 5 thru_hole oval (at -6.9 5.7 270) (size 3.5 1.9) (drill oval 2.5 0.9) (layers *.Cu *.Mask)
      (net 97 Board_4-GND))
    (pad "" np_thru_hole circle (at -6.9 -2.3 270) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -6.9 2.3 270) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_USB.3dshapes/USB_A_CNCTech_1001-011-01101_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "D:/Robotarna/Semafor/hw/USB_A_female_CNCTECH v2.step"
      (offset (xyz 11.5 0 -0.3))
      (scale (xyz 1 1 1))
      (rotate (xyz 180 0 90))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer B.Cu) (tedit 5A02FF57)
    (at 96.675001 134.605028 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at -2.905 -0.955 270) (layer B.SilkS))
    (fp_text value BC817 (at 0 -2.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 106 "Board_4-Net-(Q1-Pad1)"))
    (pad 2 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 97 Board_4-GND))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 107 "Board_4-Net-(Q1-Pad3)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer B.Cu) (tedit 5A02FF57)
    (at 100.485001 134.605028 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q2 (at -2.905 -0.955 270) (layer B.SilkS))
    (fp_text value BC817 (at 0 -2.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 108 "Board_4-Net-(Q2-Pad1)"))
    (pad 2 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 97 Board_4-GND))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 109 "Board_4-Net-(Q2-Pad3)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer B.Cu) (tedit 5A02FF57)
    (at 92.865001 134.605028 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q3 (at -2.905 -0.955 90) (layer B.SilkS))
    (fp_text value BC817 (at 0 -2.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 110 "Board_4-Net-(Q3-Pad1)"))
    (pad 2 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 97 Board_4-GND))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 111 "Board_4-Net-(Q3-Pad3)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module semaforBoard:Robotarna (layer F.Cu) (tedit 0)
    (at 72.352001 135.732028)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module semaforBoard:Helceletka (layer F.Cu) (tedit 0)
    (at 80.480001 140.050028)
    (fp_text reference G2 (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module semaforBoard:Robotarna (layer B.Cu) (tedit 0)
    (at 64.097001 127.985028 180)
    (fp_text reference G1 (at 0 0) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer B.SilkS) hide)
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 91.910001 129.672528 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C2 (at 0 1.82 90) (layer B.SilkS))
    (fp_text value 100nF (at 0 -1.82 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 119 Board_4-RESET))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 97 Board_4-GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 83.020001 139.197528 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C4 (at -3.3925 0 90) (layer B.SilkS))
    (fp_text value 100nF (at 0 -1.82 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 91 Board_4-+3V3))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 97 Board_4-GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 79.210001 130.942528 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C3 (at 3.5925 0 90) (layer B.SilkS))
    (fp_text value 22pF (at 0 -1.82 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 101 "Board_4-Net-(C3-Pad1)"))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 97 Board_4-GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 76.035001 130.942528 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C5 (at 3.5925 0 90) (layer B.SilkS))
    (fp_text value 22pF (at 0 -1.82 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 102 "Board_4-Net-(C5-Pad1)"))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 97 Board_4-GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer B.Cu) (tedit 5A02FF57)
    (at 89.050001 134.605028 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q4 (at -2.905 -0.95 90) (layer B.SilkS))
    (fp_text value BC817 (at 0 -2.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 96 Board_4-DTR))
    (pad 2 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 120 Board_4-RTS))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 119 Board_4-RESET))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer B.Cu) (tedit 5A02FF57)
    (at 85.240001 134.605028 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q5 (at 0.27 -2.855 90) (layer B.SilkS))
    (fp_text value BC817 (at 0 -2.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 120 Board_4-RTS))
    (pad 2 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 96 Board_4-DTR))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 93 Board_4-BUTTON))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 88.100001 129.672528 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R10 (at 0 1.82 270) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.82 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 119 Board_4-RESET))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 91 Board_4-+3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-16_3.9x9.9mm_P1.27mm (layer B.Cu) (tedit 5D9F72B1)
    (at 77.875001 138.780028)
    (descr "SOIC, 16 Pin (JEDEC MS-012AC, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U3 (at 0.065 6.35) (layer B.SilkS))
    (fp_text value CH340G (at 0 -5.9) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -2.475 4.445) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 97 Board_4-GND))
    (pad 2 smd roundrect (at -2.475 3.175) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 113 "Board_4-Net-(R9-Pad2)"))
    (pad 3 smd roundrect (at -2.475 1.905) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 112 "Board_4-Net-(R8-Pad2)"))
    (pad 4 smd roundrect (at -2.475 0.635) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 91 Board_4-+3V3))
    (pad 5 smd roundrect (at -2.475 -0.635) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 94 Board_4-D+))
    (pad 6 smd roundrect (at -2.475 -1.905) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 95 Board_4-D-))
    (pad 7 smd roundrect (at -2.475 -3.175) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 101 "Board_4-Net-(C3-Pad1)"))
    (pad 8 smd roundrect (at -2.475 -4.445) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 102 "Board_4-Net-(C5-Pad1)"))
    (pad 9 smd roundrect (at 2.475 -4.445) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 118 "Board_4-Net-(U3-Pad9)"))
    (pad 10 smd roundrect (at 2.475 -3.175) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 114 "Board_4-Net-(U3-Pad10)"))
    (pad 11 smd roundrect (at 2.475 -1.905) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 115 "Board_4-Net-(U3-Pad11)"))
    (pad 12 smd roundrect (at 2.475 -0.635) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 116 "Board_4-Net-(U3-Pad12)"))
    (pad 13 smd roundrect (at 2.475 0.635) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 96 Board_4-DTR))
    (pad 14 smd roundrect (at 2.475 1.905) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 120 Board_4-RTS))
    (pad 15 smd roundrect (at 2.475 3.175) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 117 "Board_4-Net-(U3-Pad15)"))
    (pad 16 smd roundrect (at 2.475 4.445) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 91 Board_4-+3V3))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-16_3.9x9.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystal:Crystal_HC49-4H_Vertical (layer B.Cu) (tedit 5A1AD3B7)
    (at 68.850001 138.780028 180)
    (descr "Crystal THT HC-49-4H http://5hertz.com/pdfs/04404_D.pdf")
    (tags "THT crystalHC-49-4H")
    (fp_text reference Y1 (at 1.07 3.525) (layer B.SilkS))
    (fp_text value Crystal (at 2.44 -3.525) (layer B.Fab))
    (fp_text user %R (at 2.44 0) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 101 "Board_4-Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 4.88 0 180) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 102 "Board_4-Net-(C5-Pad1)"))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_HC49-4H_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D10.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 54.445001 131.795028)
    (descr "LED, diameter 10.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LED10-4500RT%23KIN.pdf")
    (tags "LED diameter 10.0mm 2 pins")
    (fp_text reference D1 (at 1.27 -1.905) (layer F.SilkS))
    (fp_text value LED (at 1.27 6.56) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 103 "Board_4-Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 92 Board_4-+5V))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D10.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D10.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 54.445001 143.225028)
    (descr "LED, diameter 10.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LED10-4500RT%23KIN.pdf")
    (tags "LED diameter 10.0mm 2 pins")
    (fp_text reference D2 (at 1.27 -1.905) (layer F.SilkS))
    (fp_text value LED (at 1.27 6.56) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 103 "Board_4-Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 92 Board_4-+5V))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D10.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D10.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 70.955001 131.795028)
    (descr "LED, diameter 10.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LED10-4500RT%23KIN.pdf")
    (tags "LED diameter 10.0mm 2 pins")
    (fp_text reference D3 (at 1.27 -1.905) (layer F.SilkS))
    (fp_text value LED (at 1.27 6.56) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 104 "Board_4-Net-(D3-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 92 Board_4-+5V))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D10.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D10.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 82.385001 131.795028)
    (descr "LED, diameter 10.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LED10-4500RT%23KIN.pdf")
    (tags "LED diameter 10.0mm 2 pins")
    (fp_text reference D4 (at 1.27 -1.905) (layer F.SilkS))
    (fp_text value LED (at 1.27 6.56) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 104 "Board_4-Net-(D3-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 92 Board_4-+5V))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D10.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D10.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 98.895001 131.795028)
    (descr "LED, diameter 10.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LED10-4500RT%23KIN.pdf")
    (tags "LED diameter 10.0mm 2 pins")
    (fp_text reference D5 (at 1.27 -1.905) (layer F.SilkS))
    (fp_text value LED (at 1.27 6.56) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 105 "Board_4-Net-(D5-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 92 Board_4-+5V))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D10.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D10.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 98.895001 143.225028)
    (descr "LED, diameter 10.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LED10-4500RT%23KIN.pdf")
    (tags "LED diameter 10.0mm 2 pins")
    (fp_text reference D6 (at 1.27 -1.905) (layer F.SilkS))
    (fp_text value LED (at 1.27 6.56) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 105 "Board_4-Net-(D5-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 92 Board_4-+5V))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D10.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module semaforBoard:PinHeader_1x02_P2.54mm_Vertical (layer B.Cu) (tedit 5EE4CC18)
    (at 98.895001 145.765028 270)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J1 (at 0 2.33 90) (layer B.SilkS))
    (fp_text value RESET (at 0 -4.87 90) (layer B.Fab))
    (fp_text user %R (at 0 -1.27 180) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 119 Board_4-RESET))
    (pad 2 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 97 Board_4-GND))
  )
  (module Capacitor_THT:CP_Radial_D6.3mm_P2.50mm (layer B.Cu) (tedit 5AE50EF0)
    (at 62.700001 107.070019)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (fp_text reference C1 (at -2.54 -1.905 180) (layer B.SilkS))
    (fp_text value 47uF (at 1.25 -4.4 180) (layer B.Fab))
    (fp_text user %R (at 1.25 0 180) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 61 Board_3-+3V3))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 67 Board_3-GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 97.625001 113.837519 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0.8525 -1.905 90) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.82 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 76 "Board_3-Net-(Q1-Pad1)"))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 68 Board_3-LED-A))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 101.435001 113.837519 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at 0 -1.905 90) (layer B.SilkS))
    (fp_text value 33k (at 0 -1.82 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 78 "Board_3-Net-(Q2-Pad1)"))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 69 Board_3-LED-B))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 93.815001 113.837519 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at -0.8525 1.905 90) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.82 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 80 "Board_3-Net-(Q3-Pad1)"))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 70 Board_3-LED-C))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 60.160001 119.553019 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at 0 1.82 90) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.82 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 63 Board_3-BUTTON))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 61 Board_3-+3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 95.720001 104.312519 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R5 (at 0 1.82 90) (layer B.Fab))
    (fp_text value 75R (at 0 -1.82 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 73 "Board_3-Net-(D1-Pad1)"))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 77 "Board_3-Net-(Q1-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 83.437001 103.895019)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R6 (at 0 1.82) (layer B.Fab))
    (fp_text value 75R (at 0 -1.82) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 79 "Board_3-Net-(Q2-Pad3)"))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 74 "Board_3-Net-(D3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 99.947001 103.895019 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R7 (at 0 1.82) (layer B.SilkS))
    (fp_text value 75R (at 0 -1.82) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0 180) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 75 "Board_3-Net-(D5-Pad1)"))
    (pad 2 smd roundrect (at 1.4875 0 180) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 81 "Board_3-Net-(Q3-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 86.195001 113.837519 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R8 (at -0.8525 1.905 90) (layer B.SilkS))
    (fp_text value 1k (at 0 -1.82 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 68 Board_3-LED-A))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 82 "Board_3-Net-(R8-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 90.005001 113.837519 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R9 (at 0.8525 -1.905 90) (layer B.Fab))
    (fp_text value 1k (at 0 -1.82 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 70 Board_3-LED-C))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 83 "Board_3-Net-(R9-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_THT:SW_PUSH_6mm (layer F.Cu) (tedit 5A02FE31)
    (at 69.685001 121.675019 180)
    (descr https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "tact sw push 6mm")
    (fp_text reference SW1 (at 9.398 -0.635) (layer F.Fab))
    (fp_text value SW_Push (at 3.75 6.7) (layer F.Fab))
    (fp_text user %R (at 3.25 2.25) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 4.5 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 67 Board_3-GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 63 Board_3-BUTTON))
    (pad 2 thru_hole circle (at 6.5 4.5 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 67 Board_3-GND))
    (pad 1 thru_hole circle (at 6.5 0 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 63 Board_3-BUTTON))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_PUSH_6mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-223-3_TabPin2 (layer B.Cu) (tedit 5A02FF57)
    (at 55.690001 112.150019 180)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U2 (at 3.277 2.921) (layer B.SilkS))
    (fp_text value AMS1117-3.3 (at 0 -4.5) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd rect (at 3.15 0 180) (size 2 3.8) (layers B.Cu B.Paste B.Mask)
      (net 61 Board_3-+3V3))
    (pad 2 smd rect (at -3.15 0 180) (size 2 1.5) (layers B.Cu B.Paste B.Mask)
      (net 61 Board_3-+3V3))
    (pad 3 smd rect (at -3.15 -2.3 180) (size 2 1.5) (layers B.Cu B.Paste B.Mask)
      (net 62 Board_3-+5V))
    (pad 1 smd rect (at -3.15 2.3 180) (size 2 1.5) (layers B.Cu B.Paste B.Mask)
      (net 67 Board_3-GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module semaforBoard:ESP-01 (layer B.Cu) (tedit 5EC82F3F)
    (at 91.275001 110.880019 90)
    (fp_text reference U1 (at -8.89 4.445 90) (layer B.Fab))
    (fp_text value ESP-01 (at -12.065 -1.27 180) (layer B.SilkS))
    (pad 1 thru_hole circle (at -10.16 -5.08 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 61 Board_3-+3V3))
    (pad 2 thru_hole circle (at -7.62 2.54 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 67 Board_3-GND))
    (pad 3 thru_hole circle (at -10.16 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 61 Board_3-+3V3))
    (pad 4 thru_hole circle (at -10.16 -2.54 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 89 Board_3-RESET))
    (pad 5 thru_hole circle (at -7.62 -2.54 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 63 Board_3-BUTTON))
    (pad 6 thru_hole circle (at -10.16 2.54 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 68 Board_3-LED-A))
    (pad 7 thru_hole circle (at -7.62 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 69 Board_3-LED-B))
    (pad 8 thru_hole circle (at -7.62 -5.08 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 70 Board_3-LED-C))
    (model "D:/Robotarna/Semafor/hw/ESP-01-fixed v3.step"
      (offset (xyz 0.8 -1.2 3))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module semaforBoard:USB_A_CNCTech_1001-011-01101_Horizontal (layer F.Cu) (tedit 5EC84A2B)
    (at 77.925001 127.305019 270)
    (descr "USB type A Plug, Horizontal, http://cnctech.us/pdfs/1001-011-01101.pdf")
    (tags USB-A)
    (attr smd)
    (fp_text reference J3 (at -6.9 -8 90) (layer F.Fab))
    (fp_text value USB_A (at -4.995 -0.015) (layer F.Fab))
    (fp_text user "PCB Edge" (at -4.55 -0.05) (layer Dwgs.User))
    (fp_text user %R (at -6 0) (layer F.Fab))
    (pad 2 smd rect (at -9.65 -1 270) (size 2.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 65 Board_3-D-))
    (pad 3 smd rect (at -9.65 1 270) (size 2.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 64 Board_3-D+))
    (pad 1 smd rect (at -9.65 -3.5 270) (size 2.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 62 Board_3-+5V))
    (pad 4 smd rect (at -9.65 3.5 270) (size 2.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 67 Board_3-GND))
    (pad 5 thru_hole oval (at -6.9 -5.7 270) (size 3.5 1.9) (drill oval 2.5 0.9) (layers *.Cu *.Mask)
      (net 67 Board_3-GND))
    (pad 5 thru_hole oval (at -6.9 5.7 270) (size 3.5 1.9) (drill oval 2.5 0.9) (layers *.Cu *.Mask)
      (net 67 Board_3-GND))
    (pad "" np_thru_hole circle (at -6.9 -2.3 270) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -6.9 2.3 270) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_USB.3dshapes/USB_A_CNCTech_1001-011-01101_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "D:/Robotarna/Semafor/hw/USB_A_female_CNCTECH v2.step"
      (offset (xyz 11.5 0 -0.3))
      (scale (xyz 1 1 1))
      (rotate (xyz 180 0 90))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer B.Cu) (tedit 5A02FF57)
    (at 96.675001 109.245019 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at -2.905 -0.955 270) (layer B.SilkS))
    (fp_text value BC817 (at 0 -2.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 76 "Board_3-Net-(Q1-Pad1)"))
    (pad 2 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 67 Board_3-GND))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 77 "Board_3-Net-(Q1-Pad3)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer B.Cu) (tedit 5A02FF57)
    (at 100.485001 109.245019 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q2 (at -2.905 -0.955 270) (layer B.SilkS))
    (fp_text value BC817 (at 0 -2.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 78 "Board_3-Net-(Q2-Pad1)"))
    (pad 2 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 67 Board_3-GND))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 79 "Board_3-Net-(Q2-Pad3)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer B.Cu) (tedit 5A02FF57)
    (at 92.865001 109.245019 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q3 (at -2.905 -0.955 90) (layer B.SilkS))
    (fp_text value BC817 (at 0 -2.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 80 "Board_3-Net-(Q3-Pad1)"))
    (pad 2 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 67 Board_3-GND))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 81 "Board_3-Net-(Q3-Pad3)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module semaforBoard:Robotarna (layer F.Cu) (tedit 0)
    (at 72.352001 110.372019)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module semaforBoard:Helceletka (layer F.Cu) (tedit 0)
    (at 80.480001 114.690019)
    (fp_text reference G2 (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module semaforBoard:Robotarna (layer B.Cu) (tedit 0)
    (at 64.097001 102.625019 180)
    (fp_text reference G1 (at 0 0) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer B.SilkS) hide)
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 91.910001 104.312519 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C2 (at 0 1.82 90) (layer B.SilkS))
    (fp_text value 100nF (at 0 -1.82 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 89 Board_3-RESET))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 67 Board_3-GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 83.020001 113.837519 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C4 (at -3.3925 0 90) (layer B.SilkS))
    (fp_text value 100nF (at 0 -1.82 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 61 Board_3-+3V3))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 67 Board_3-GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 79.210001 105.582519 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C3 (at 3.5925 0 90) (layer B.SilkS))
    (fp_text value 22pF (at 0 -1.82 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 71 "Board_3-Net-(C3-Pad1)"))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 67 Board_3-GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 76.035001 105.582519 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C5 (at 3.5925 0 90) (layer B.SilkS))
    (fp_text value 22pF (at 0 -1.82 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 72 "Board_3-Net-(C5-Pad1)"))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 67 Board_3-GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer B.Cu) (tedit 5A02FF57)
    (at 89.050001 109.245019 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q4 (at -2.905 -0.95 90) (layer B.SilkS))
    (fp_text value BC817 (at 0 -2.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 66 Board_3-DTR))
    (pad 2 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 90 Board_3-RTS))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 89 Board_3-RESET))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer B.Cu) (tedit 5A02FF57)
    (at 85.240001 109.245019 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q5 (at 0.27 -2.855 90) (layer B.SilkS))
    (fp_text value BC817 (at 0 -2.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 90 Board_3-RTS))
    (pad 2 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 66 Board_3-DTR))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 63 Board_3-BUTTON))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 88.100001 104.312519 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R10 (at 0 1.82 270) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.82 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 89 Board_3-RESET))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 61 Board_3-+3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-16_3.9x9.9mm_P1.27mm (layer B.Cu) (tedit 5D9F72B1)
    (at 77.875001 113.420019)
    (descr "SOIC, 16 Pin (JEDEC MS-012AC, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U3 (at 0.065 6.35) (layer B.SilkS))
    (fp_text value CH340G (at 0 -5.9) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -2.475 4.445) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 67 Board_3-GND))
    (pad 2 smd roundrect (at -2.475 3.175) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 83 "Board_3-Net-(R9-Pad2)"))
    (pad 3 smd roundrect (at -2.475 1.905) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 82 "Board_3-Net-(R8-Pad2)"))
    (pad 4 smd roundrect (at -2.475 0.635) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 61 Board_3-+3V3))
    (pad 5 smd roundrect (at -2.475 -0.635) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 64 Board_3-D+))
    (pad 6 smd roundrect (at -2.475 -1.905) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 65 Board_3-D-))
    (pad 7 smd roundrect (at -2.475 -3.175) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 71 "Board_3-Net-(C3-Pad1)"))
    (pad 8 smd roundrect (at -2.475 -4.445) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 72 "Board_3-Net-(C5-Pad1)"))
    (pad 9 smd roundrect (at 2.475 -4.445) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 88 "Board_3-Net-(U3-Pad9)"))
    (pad 10 smd roundrect (at 2.475 -3.175) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 84 "Board_3-Net-(U3-Pad10)"))
    (pad 11 smd roundrect (at 2.475 -1.905) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 85 "Board_3-Net-(U3-Pad11)"))
    (pad 12 smd roundrect (at 2.475 -0.635) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 86 "Board_3-Net-(U3-Pad12)"))
    (pad 13 smd roundrect (at 2.475 0.635) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 66 Board_3-DTR))
    (pad 14 smd roundrect (at 2.475 1.905) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 90 Board_3-RTS))
    (pad 15 smd roundrect (at 2.475 3.175) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 87 "Board_3-Net-(U3-Pad15)"))
    (pad 16 smd roundrect (at 2.475 4.445) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 61 Board_3-+3V3))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-16_3.9x9.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystal:Crystal_HC49-4H_Vertical (layer B.Cu) (tedit 5A1AD3B7)
    (at 68.850001 113.420019 180)
    (descr "Crystal THT HC-49-4H http://5hertz.com/pdfs/04404_D.pdf")
    (tags "THT crystalHC-49-4H")
    (fp_text reference Y1 (at 1.07 3.525) (layer B.SilkS))
    (fp_text value Crystal (at 2.44 -3.525) (layer B.Fab))
    (fp_text user %R (at 2.44 0) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 71 "Board_3-Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 4.88 0 180) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 72 "Board_3-Net-(C5-Pad1)"))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_HC49-4H_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D10.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 54.445001 106.435019)
    (descr "LED, diameter 10.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LED10-4500RT%23KIN.pdf")
    (tags "LED diameter 10.0mm 2 pins")
    (fp_text reference D1 (at 1.27 -1.905) (layer F.SilkS))
    (fp_text value LED (at 1.27 6.56) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 73 "Board_3-Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 62 Board_3-+5V))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D10.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D10.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 54.445001 117.865019)
    (descr "LED, diameter 10.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LED10-4500RT%23KIN.pdf")
    (tags "LED diameter 10.0mm 2 pins")
    (fp_text reference D2 (at 1.27 -1.905) (layer F.SilkS))
    (fp_text value LED (at 1.27 6.56) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 73 "Board_3-Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 62 Board_3-+5V))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D10.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D10.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 70.955001 106.435019)
    (descr "LED, diameter 10.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LED10-4500RT%23KIN.pdf")
    (tags "LED diameter 10.0mm 2 pins")
    (fp_text reference D3 (at 1.27 -1.905) (layer F.SilkS))
    (fp_text value LED (at 1.27 6.56) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 74 "Board_3-Net-(D3-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 62 Board_3-+5V))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D10.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D10.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 82.385001 106.435019)
    (descr "LED, diameter 10.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LED10-4500RT%23KIN.pdf")
    (tags "LED diameter 10.0mm 2 pins")
    (fp_text reference D4 (at 1.27 -1.905) (layer F.SilkS))
    (fp_text value LED (at 1.27 6.56) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 74 "Board_3-Net-(D3-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 62 Board_3-+5V))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D10.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D10.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 98.895001 106.435019)
    (descr "LED, diameter 10.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LED10-4500RT%23KIN.pdf")
    (tags "LED diameter 10.0mm 2 pins")
    (fp_text reference D5 (at 1.27 -1.905) (layer F.SilkS))
    (fp_text value LED (at 1.27 6.56) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 75 "Board_3-Net-(D5-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 62 Board_3-+5V))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D10.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D10.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 98.895001 117.865019)
    (descr "LED, diameter 10.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LED10-4500RT%23KIN.pdf")
    (tags "LED diameter 10.0mm 2 pins")
    (fp_text reference D6 (at 1.27 -1.905) (layer F.SilkS))
    (fp_text value LED (at 1.27 6.56) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 75 "Board_3-Net-(D5-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 62 Board_3-+5V))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D10.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module semaforBoard:PinHeader_1x02_P2.54mm_Vertical (layer B.Cu) (tedit 5EE4CC18)
    (at 98.895001 120.405019 270)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J1 (at 0 2.33 90) (layer B.SilkS))
    (fp_text value RESET (at 0 -4.87 90) (layer B.Fab))
    (fp_text user %R (at 0 -1.27 180) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 89 Board_3-RESET))
    (pad 2 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 67 Board_3-GND))
  )
  (module Capacitor_THT:CP_Radial_D6.3mm_P2.50mm (layer B.Cu) (tedit 5AE50EF0)
    (at 62.700001 81.71001)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (fp_text reference C1 (at -2.54 -1.905 180) (layer B.SilkS))
    (fp_text value 47uF (at 1.25 -4.4 180) (layer B.Fab))
    (fp_text user %R (at 1.25 0 180) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 Board_2-+3V3))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 Board_2-GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 97.625001 88.47751 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0.8525 -1.905 90) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.82 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 46 "Board_2-Net-(Q1-Pad1)"))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 38 Board_2-LED-A))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 101.435001 88.47751 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at 0 -1.905 90) (layer B.SilkS))
    (fp_text value 33k (at 0 -1.82 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 48 "Board_2-Net-(Q2-Pad1)"))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 39 Board_2-LED-B))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 93.815001 88.47751 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at -0.8525 1.905 90) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.82 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 50 "Board_2-Net-(Q3-Pad1)"))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 40 Board_2-LED-C))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 60.160001 94.19301 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at 0 1.82 90) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.82 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 33 Board_2-BUTTON))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 31 Board_2-+3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 95.720001 78.95251 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R5 (at 0 1.82 90) (layer B.Fab))
    (fp_text value 75R (at 0 -1.82 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 43 "Board_2-Net-(D1-Pad1)"))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 47 "Board_2-Net-(Q1-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 83.437001 78.53501)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R6 (at 0 1.82) (layer B.Fab))
    (fp_text value 75R (at 0 -1.82) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 49 "Board_2-Net-(Q2-Pad3)"))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 44 "Board_2-Net-(D3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 99.947001 78.53501 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R7 (at 0 1.82) (layer B.SilkS))
    (fp_text value 75R (at 0 -1.82) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0 180) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 45 "Board_2-Net-(D5-Pad1)"))
    (pad 2 smd roundrect (at 1.4875 0 180) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 51 "Board_2-Net-(Q3-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 86.195001 88.47751 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R8 (at -0.8525 1.905 90) (layer B.SilkS))
    (fp_text value 1k (at 0 -1.82 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 38 Board_2-LED-A))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 52 "Board_2-Net-(R8-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 90.005001 88.47751 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R9 (at 0.8525 -1.905 90) (layer B.Fab))
    (fp_text value 1k (at 0 -1.82 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 40 Board_2-LED-C))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 53 "Board_2-Net-(R9-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_THT:SW_PUSH_6mm (layer F.Cu) (tedit 5A02FE31)
    (at 69.685001 96.31501 180)
    (descr https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "tact sw push 6mm")
    (fp_text reference SW1 (at 9.398 -0.635) (layer F.Fab))
    (fp_text value SW_Push (at 3.75 6.7) (layer F.Fab))
    (fp_text user %R (at 3.25 2.25) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 4.5 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 37 Board_2-GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 33 Board_2-BUTTON))
    (pad 2 thru_hole circle (at 6.5 4.5 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 37 Board_2-GND))
    (pad 1 thru_hole circle (at 6.5 0 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 33 Board_2-BUTTON))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_PUSH_6mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-223-3_TabPin2 (layer B.Cu) (tedit 5A02FF57)
    (at 55.690001 86.79001 180)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U2 (at 3.277 2.921) (layer B.SilkS))
    (fp_text value AMS1117-3.3 (at 0 -4.5) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd rect (at 3.15 0 180) (size 2 3.8) (layers B.Cu B.Paste B.Mask)
      (net 31 Board_2-+3V3))
    (pad 2 smd rect (at -3.15 0 180) (size 2 1.5) (layers B.Cu B.Paste B.Mask)
      (net 31 Board_2-+3V3))
    (pad 3 smd rect (at -3.15 -2.3 180) (size 2 1.5) (layers B.Cu B.Paste B.Mask)
      (net 32 Board_2-+5V))
    (pad 1 smd rect (at -3.15 2.3 180) (size 2 1.5) (layers B.Cu B.Paste B.Mask)
      (net 37 Board_2-GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module semaforBoard:ESP-01 (layer B.Cu) (tedit 5EC82F3F)
    (at 91.275001 85.52001 90)
    (fp_text reference U1 (at -8.89 4.445 90) (layer B.Fab))
    (fp_text value ESP-01 (at -12.065 -1.27 180) (layer B.SilkS))
    (pad 1 thru_hole circle (at -10.16 -5.08 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 31 Board_2-+3V3))
    (pad 2 thru_hole circle (at -7.62 2.54 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 37 Board_2-GND))
    (pad 3 thru_hole circle (at -10.16 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 31 Board_2-+3V3))
    (pad 4 thru_hole circle (at -10.16 -2.54 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 59 Board_2-RESET))
    (pad 5 thru_hole circle (at -7.62 -2.54 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 33 Board_2-BUTTON))
    (pad 6 thru_hole circle (at -10.16 2.54 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 38 Board_2-LED-A))
    (pad 7 thru_hole circle (at -7.62 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 39 Board_2-LED-B))
    (pad 8 thru_hole circle (at -7.62 -5.08 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 40 Board_2-LED-C))
    (model "D:/Robotarna/Semafor/hw/ESP-01-fixed v3.step"
      (offset (xyz 0.8 -1.2 3))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module semaforBoard:USB_A_CNCTech_1001-011-01101_Horizontal (layer F.Cu) (tedit 5EC84A2B)
    (at 77.925001 101.94501 270)
    (descr "USB type A Plug, Horizontal, http://cnctech.us/pdfs/1001-011-01101.pdf")
    (tags USB-A)
    (attr smd)
    (fp_text reference J3 (at -6.9 -8 90) (layer F.Fab))
    (fp_text value USB_A (at -4.995 -0.015) (layer F.Fab))
    (fp_text user "PCB Edge" (at -4.55 -0.05) (layer Dwgs.User))
    (fp_text user %R (at -6 0) (layer F.Fab))
    (pad 2 smd rect (at -9.65 -1 270) (size 2.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 35 Board_2-D-))
    (pad 3 smd rect (at -9.65 1 270) (size 2.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 34 Board_2-D+))
    (pad 1 smd rect (at -9.65 -3.5 270) (size 2.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 32 Board_2-+5V))
    (pad 4 smd rect (at -9.65 3.5 270) (size 2.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 37 Board_2-GND))
    (pad 5 thru_hole oval (at -6.9 -5.7 270) (size 3.5 1.9) (drill oval 2.5 0.9) (layers *.Cu *.Mask)
      (net 37 Board_2-GND))
    (pad 5 thru_hole oval (at -6.9 5.7 270) (size 3.5 1.9) (drill oval 2.5 0.9) (layers *.Cu *.Mask)
      (net 37 Board_2-GND))
    (pad "" np_thru_hole circle (at -6.9 -2.3 270) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -6.9 2.3 270) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_USB.3dshapes/USB_A_CNCTech_1001-011-01101_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "D:/Robotarna/Semafor/hw/USB_A_female_CNCTECH v2.step"
      (offset (xyz 11.5 0 -0.3))
      (scale (xyz 1 1 1))
      (rotate (xyz 180 0 90))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer B.Cu) (tedit 5A02FF57)
    (at 96.675001 83.88501 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at -2.905 -0.955 270) (layer B.SilkS))
    (fp_text value BC817 (at 0 -2.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 46 "Board_2-Net-(Q1-Pad1)"))
    (pad 2 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 37 Board_2-GND))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 47 "Board_2-Net-(Q1-Pad3)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer B.Cu) (tedit 5A02FF57)
    (at 100.485001 83.88501 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q2 (at -2.905 -0.955 270) (layer B.SilkS))
    (fp_text value BC817 (at 0 -2.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 48 "Board_2-Net-(Q2-Pad1)"))
    (pad 2 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 37 Board_2-GND))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 49 "Board_2-Net-(Q2-Pad3)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer B.Cu) (tedit 5A02FF57)
    (at 92.865001 83.88501 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q3 (at -2.905 -0.955 90) (layer B.SilkS))
    (fp_text value BC817 (at 0 -2.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 50 "Board_2-Net-(Q3-Pad1)"))
    (pad 2 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 37 Board_2-GND))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 51 "Board_2-Net-(Q3-Pad3)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module semaforBoard:Robotarna (layer F.Cu) (tedit 0)
    (at 72.352001 85.01201)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module semaforBoard:Helceletka (layer F.Cu) (tedit 0)
    (at 80.480001 89.33001)
    (fp_text reference G2 (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module semaforBoard:Robotarna (layer B.Cu) (tedit 0)
    (at 64.097001 77.26501 180)
    (fp_text reference G1 (at 0 0) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer B.SilkS) hide)
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 91.910001 78.95251 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C2 (at 0 1.82 90) (layer B.SilkS))
    (fp_text value 100nF (at 0 -1.82 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 59 Board_2-RESET))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 37 Board_2-GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 83.020001 88.47751 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C4 (at -3.3925 0 90) (layer B.SilkS))
    (fp_text value 100nF (at 0 -1.82 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 31 Board_2-+3V3))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 37 Board_2-GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 79.210001 80.22251 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C3 (at 3.5925 0 90) (layer B.SilkS))
    (fp_text value 22pF (at 0 -1.82 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 41 "Board_2-Net-(C3-Pad1)"))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 37 Board_2-GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 76.035001 80.22251 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C5 (at 3.5925 0 90) (layer B.SilkS))
    (fp_text value 22pF (at 0 -1.82 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 42 "Board_2-Net-(C5-Pad1)"))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 37 Board_2-GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer B.Cu) (tedit 5A02FF57)
    (at 89.050001 83.88501 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q4 (at -2.905 -0.95 90) (layer B.SilkS))
    (fp_text value BC817 (at 0 -2.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 36 Board_2-DTR))
    (pad 2 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 60 Board_2-RTS))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 59 Board_2-RESET))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer B.Cu) (tedit 5A02FF57)
    (at 85.240001 83.88501 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q5 (at 0.27 -2.855 90) (layer B.SilkS))
    (fp_text value BC817 (at 0 -2.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 60 Board_2-RTS))
    (pad 2 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 36 Board_2-DTR))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 33 Board_2-BUTTON))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 88.100001 78.95251 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R10 (at 0 1.82 270) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.82 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 59 Board_2-RESET))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 31 Board_2-+3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-16_3.9x9.9mm_P1.27mm (layer B.Cu) (tedit 5D9F72B1)
    (at 77.875001 88.06001)
    (descr "SOIC, 16 Pin (JEDEC MS-012AC, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U3 (at 0.065 6.35) (layer B.SilkS))
    (fp_text value CH340G (at 0 -5.9) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -2.475 4.445) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 37 Board_2-GND))
    (pad 2 smd roundrect (at -2.475 3.175) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 53 "Board_2-Net-(R9-Pad2)"))
    (pad 3 smd roundrect (at -2.475 1.905) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 52 "Board_2-Net-(R8-Pad2)"))
    (pad 4 smd roundrect (at -2.475 0.635) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 31 Board_2-+3V3))
    (pad 5 smd roundrect (at -2.475 -0.635) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 34 Board_2-D+))
    (pad 6 smd roundrect (at -2.475 -1.905) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 35 Board_2-D-))
    (pad 7 smd roundrect (at -2.475 -3.175) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 41 "Board_2-Net-(C3-Pad1)"))
    (pad 8 smd roundrect (at -2.475 -4.445) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 42 "Board_2-Net-(C5-Pad1)"))
    (pad 9 smd roundrect (at 2.475 -4.445) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 58 "Board_2-Net-(U3-Pad9)"))
    (pad 10 smd roundrect (at 2.475 -3.175) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 54 "Board_2-Net-(U3-Pad10)"))
    (pad 11 smd roundrect (at 2.475 -1.905) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 55 "Board_2-Net-(U3-Pad11)"))
    (pad 12 smd roundrect (at 2.475 -0.635) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 56 "Board_2-Net-(U3-Pad12)"))
    (pad 13 smd roundrect (at 2.475 0.635) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 36 Board_2-DTR))
    (pad 14 smd roundrect (at 2.475 1.905) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 60 Board_2-RTS))
    (pad 15 smd roundrect (at 2.475 3.175) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 57 "Board_2-Net-(U3-Pad15)"))
    (pad 16 smd roundrect (at 2.475 4.445) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 31 Board_2-+3V3))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-16_3.9x9.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystal:Crystal_HC49-4H_Vertical (layer B.Cu) (tedit 5A1AD3B7)
    (at 68.850001 88.06001 180)
    (descr "Crystal THT HC-49-4H http://5hertz.com/pdfs/04404_D.pdf")
    (tags "THT crystalHC-49-4H")
    (fp_text reference Y1 (at 1.07 3.525) (layer B.SilkS))
    (fp_text value Crystal (at 2.44 -3.525) (layer B.Fab))
    (fp_text user %R (at 2.44 0) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 "Board_2-Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 4.88 0 180) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 "Board_2-Net-(C5-Pad1)"))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_HC49-4H_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D10.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 54.445001 81.07501)
    (descr "LED, diameter 10.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LED10-4500RT%23KIN.pdf")
    (tags "LED diameter 10.0mm 2 pins")
    (fp_text reference D1 (at 1.27 -1.905) (layer F.SilkS))
    (fp_text value LED (at 1.27 6.56) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 43 "Board_2-Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 32 Board_2-+5V))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D10.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D10.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 54.445001 92.50501)
    (descr "LED, diameter 10.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LED10-4500RT%23KIN.pdf")
    (tags "LED diameter 10.0mm 2 pins")
    (fp_text reference D2 (at 1.27 -1.905) (layer F.SilkS))
    (fp_text value LED (at 1.27 6.56) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 43 "Board_2-Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 32 Board_2-+5V))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D10.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D10.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 70.955001 81.07501)
    (descr "LED, diameter 10.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LED10-4500RT%23KIN.pdf")
    (tags "LED diameter 10.0mm 2 pins")
    (fp_text reference D3 (at 1.27 -1.905) (layer F.SilkS))
    (fp_text value LED (at 1.27 6.56) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 44 "Board_2-Net-(D3-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 32 Board_2-+5V))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D10.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D10.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 82.385001 81.07501)
    (descr "LED, diameter 10.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LED10-4500RT%23KIN.pdf")
    (tags "LED diameter 10.0mm 2 pins")
    (fp_text reference D4 (at 1.27 -1.905) (layer F.SilkS))
    (fp_text value LED (at 1.27 6.56) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 44 "Board_2-Net-(D3-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 32 Board_2-+5V))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D10.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D10.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 98.895001 81.07501)
    (descr "LED, diameter 10.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LED10-4500RT%23KIN.pdf")
    (tags "LED diameter 10.0mm 2 pins")
    (fp_text reference D5 (at 1.27 -1.905) (layer F.SilkS))
    (fp_text value LED (at 1.27 6.56) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 45 "Board_2-Net-(D5-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 32 Board_2-+5V))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D10.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D10.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 98.895001 92.50501)
    (descr "LED, diameter 10.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LED10-4500RT%23KIN.pdf")
    (tags "LED diameter 10.0mm 2 pins")
    (fp_text reference D6 (at 1.27 -1.905) (layer F.SilkS))
    (fp_text value LED (at 1.27 6.56) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 45 "Board_2-Net-(D5-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 32 Board_2-+5V))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D10.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module semaforBoard:PinHeader_1x02_P2.54mm_Vertical (layer B.Cu) (tedit 5EE4CC18)
    (at 98.895001 95.04501 270)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J1 (at 0 2.33 90) (layer B.SilkS))
    (fp_text value RESET (at 0 -4.87 90) (layer B.Fab))
    (fp_text user %R (at 0 -1.27 180) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 59 Board_2-RESET))
    (pad 2 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 Board_2-GND))
  )
  (module Capacitor_THT:CP_Radial_D6.3mm_P2.50mm (layer B.Cu) (tedit 5AE50EF0)
    (at 62.700001 56.350001)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (fp_text reference C1 (at -2.54 -1.905 180) (layer B.SilkS))
    (fp_text value 47uF (at 1.25 -4.4 180) (layer B.Fab))
    (fp_text user %R (at 1.25 0 180) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 Board_1-+3V3))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 Board_1-GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 97.625001 63.117501 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0.8525 -1.905 90) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.82 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 16 "Board_1-Net-(Q1-Pad1)"))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 8 Board_1-LED-A))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 101.435001 63.117501 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at 0 -1.905 90) (layer B.SilkS))
    (fp_text value 33k (at 0 -1.82 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 18 "Board_1-Net-(Q2-Pad1)"))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 9 Board_1-LED-B))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 93.815001 63.117501 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at -0.8525 1.905 90) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.82 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 20 "Board_1-Net-(Q3-Pad1)"))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 10 Board_1-LED-C))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 60.160001 68.833001 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at 0 1.82 90) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.82 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 3 Board_1-BUTTON))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 1 Board_1-+3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 95.720001 53.592501 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R5 (at 0 1.82 90) (layer B.Fab))
    (fp_text value 75R (at 0 -1.82 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 13 "Board_1-Net-(D1-Pad1)"))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 17 "Board_1-Net-(Q1-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 83.437001 53.175001)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R6 (at 0 1.82) (layer B.Fab))
    (fp_text value 75R (at 0 -1.82) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 19 "Board_1-Net-(Q2-Pad3)"))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 14 "Board_1-Net-(D3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 99.947001 53.175001 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R7 (at 0 1.82) (layer B.SilkS))
    (fp_text value 75R (at 0 -1.82) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0 180) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 15 "Board_1-Net-(D5-Pad1)"))
    (pad 2 smd roundrect (at 1.4875 0 180) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 21 "Board_1-Net-(Q3-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 86.195001 63.117501 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R8 (at -0.8525 1.905 90) (layer B.SilkS))
    (fp_text value 1k (at 0 -1.82 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 8 Board_1-LED-A))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 22 "Board_1-Net-(R8-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 90.005001 63.117501 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R9 (at 0.8525 -1.905 90) (layer B.Fab))
    (fp_text value 1k (at 0 -1.82 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 10 Board_1-LED-C))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 23 "Board_1-Net-(R9-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_THT:SW_PUSH_6mm (layer F.Cu) (tedit 5A02FE31)
    (at 69.685001 70.955001 180)
    (descr https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "tact sw push 6mm")
    (fp_text reference SW1 (at 9.398 -0.635) (layer F.Fab))
    (fp_text value SW_Push (at 3.75 6.7) (layer F.Fab))
    (fp_text user %R (at 3.25 2.25) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 4.5 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 7 Board_1-GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 Board_1-BUTTON))
    (pad 2 thru_hole circle (at 6.5 4.5 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 7 Board_1-GND))
    (pad 1 thru_hole circle (at 6.5 0 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 Board_1-BUTTON))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_PUSH_6mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-223-3_TabPin2 (layer B.Cu) (tedit 5A02FF57)
    (at 55.690001 61.430001 180)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U2 (at 3.277 2.921) (layer B.SilkS))
    (fp_text value AMS1117-3.3 (at 0 -4.5) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd rect (at 3.15 0 180) (size 2 3.8) (layers B.Cu B.Paste B.Mask)
      (net 1 Board_1-+3V3))
    (pad 2 smd rect (at -3.15 0 180) (size 2 1.5) (layers B.Cu B.Paste B.Mask)
      (net 1 Board_1-+3V3))
    (pad 3 smd rect (at -3.15 -2.3 180) (size 2 1.5) (layers B.Cu B.Paste B.Mask)
      (net 2 Board_1-+5V))
    (pad 1 smd rect (at -3.15 2.3 180) (size 2 1.5) (layers B.Cu B.Paste B.Mask)
      (net 7 Board_1-GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module semaforBoard:ESP-01 (layer B.Cu) (tedit 5EC82F3F)
    (at 91.275001 60.160001 90)
    (fp_text reference U1 (at -8.89 4.445 90) (layer B.Fab))
    (fp_text value ESP-01 (at -12.065 -1.27 180) (layer B.SilkS))
    (pad 1 thru_hole circle (at -10.16 -5.08 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 Board_1-+3V3))
    (pad 2 thru_hole circle (at -7.62 2.54 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 7 Board_1-GND))
    (pad 3 thru_hole circle (at -10.16 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 Board_1-+3V3))
    (pad 4 thru_hole circle (at -10.16 -2.54 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 29 Board_1-RESET))
    (pad 5 thru_hole circle (at -7.62 -2.54 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 3 Board_1-BUTTON))
    (pad 6 thru_hole circle (at -10.16 2.54 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 8 Board_1-LED-A))
    (pad 7 thru_hole circle (at -7.62 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 9 Board_1-LED-B))
    (pad 8 thru_hole circle (at -7.62 -5.08 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 10 Board_1-LED-C))
    (model "D:/Robotarna/Semafor/hw/ESP-01-fixed v3.step"
      (offset (xyz 0.8 -1.2 3))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module semaforBoard:USB_A_CNCTech_1001-011-01101_Horizontal (layer F.Cu) (tedit 5EC84A2B)
    (at 77.925001 76.585001 270)
    (descr "USB type A Plug, Horizontal, http://cnctech.us/pdfs/1001-011-01101.pdf")
    (tags USB-A)
    (attr smd)
    (fp_text reference J3 (at -6.9 -8 90) (layer F.Fab))
    (fp_text value USB_A (at -4.995 -0.015) (layer F.Fab))
    (fp_text user "PCB Edge" (at -4.55 -0.05) (layer Dwgs.User))
    (fp_text user %R (at -6 0) (layer F.Fab))
    (pad 2 smd rect (at -9.65 -1 270) (size 2.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 5 Board_1-D-))
    (pad 3 smd rect (at -9.65 1 270) (size 2.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 4 Board_1-D+))
    (pad 1 smd rect (at -9.65 -3.5 270) (size 2.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 2 Board_1-+5V))
    (pad 4 smd rect (at -9.65 3.5 270) (size 2.5 1.1) (layers F.Cu F.Paste F.Mask)
      (net 7 Board_1-GND))
    (pad 5 thru_hole oval (at -6.9 -5.7 270) (size 3.5 1.9) (drill oval 2.5 0.9) (layers *.Cu *.Mask)
      (net 7 Board_1-GND))
    (pad 5 thru_hole oval (at -6.9 5.7 270) (size 3.5 1.9) (drill oval 2.5 0.9) (layers *.Cu *.Mask)
      (net 7 Board_1-GND))
    (pad "" np_thru_hole circle (at -6.9 -2.3 270) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -6.9 2.3 270) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_USB.3dshapes/USB_A_CNCTech_1001-011-01101_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "D:/Robotarna/Semafor/hw/USB_A_female_CNCTECH v2.step"
      (offset (xyz 11.5 0 -0.3))
      (scale (xyz 1 1 1))
      (rotate (xyz 180 0 90))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer B.Cu) (tedit 5A02FF57)
    (at 96.675001 58.525001 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at -2.905 -0.955 270) (layer B.SilkS))
    (fp_text value BC817 (at 0 -2.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 16 "Board_1-Net-(Q1-Pad1)"))
    (pad 2 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 7 Board_1-GND))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 17 "Board_1-Net-(Q1-Pad3)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer B.Cu) (tedit 5A02FF57)
    (at 100.485001 58.525001 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q2 (at -2.905 -0.955 270) (layer B.SilkS))
    (fp_text value BC817 (at 0 -2.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 18 "Board_1-Net-(Q2-Pad1)"))
    (pad 2 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 7 Board_1-GND))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 19 "Board_1-Net-(Q2-Pad3)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer B.Cu) (tedit 5A02FF57)
    (at 92.865001 58.525001 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q3 (at -2.905 -0.955 90) (layer B.SilkS))
    (fp_text value BC817 (at 0 -2.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 20 "Board_1-Net-(Q3-Pad1)"))
    (pad 2 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 7 Board_1-GND))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 21 "Board_1-Net-(Q3-Pad3)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module semaforBoard:Robotarna (layer F.Cu) (tedit 0)
    (at 72.352001 59.652001)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module semaforBoard:Helceletka (layer F.Cu) (tedit 0)
    (at 80.480001 63.970001)
    (fp_text reference G2 (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module semaforBoard:Robotarna (layer B.Cu) (tedit 0)
    (at 64.097001 51.905001 180)
    (fp_text reference G1 (at 0 0) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer B.SilkS) hide)
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 91.910001 53.592501 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C2 (at 0 1.82 90) (layer B.SilkS))
    (fp_text value 100nF (at 0 -1.82 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 29 Board_1-RESET))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 7 Board_1-GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 83.020001 63.117501 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C4 (at -3.3925 0 90) (layer B.SilkS))
    (fp_text value 100nF (at 0 -1.82 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 1 Board_1-+3V3))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 7 Board_1-GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 79.210001 54.862501 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C3 (at 3.5925 0 90) (layer B.SilkS))
    (fp_text value 22pF (at 0 -1.82 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 11 "Board_1-Net-(C3-Pad1)"))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 7 Board_1-GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 76.035001 54.862501 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C5 (at 3.5925 0 90) (layer B.SilkS))
    (fp_text value 22pF (at 0 -1.82 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 12 "Board_1-Net-(C5-Pad1)"))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 7 Board_1-GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer B.Cu) (tedit 5A02FF57)
    (at 89.050001 58.525001 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q4 (at -2.905 -0.95 90) (layer B.SilkS))
    (fp_text value BC817 (at 0 -2.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 6 Board_1-DTR))
    (pad 2 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 30 Board_1-RTS))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 29 Board_1-RESET))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer B.Cu) (tedit 5A02FF57)
    (at 85.240001 58.525001 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q5 (at 0.27 -2.855 90) (layer B.SilkS))
    (fp_text value BC817 (at 0 -2.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 30 Board_1-RTS))
    (pad 2 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 6 Board_1-DTR))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 3 Board_1-BUTTON))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 88.100001 53.592501 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R10 (at 0 1.82 270) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.82 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 29 Board_1-RESET))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 1 Board_1-+3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-16_3.9x9.9mm_P1.27mm (layer B.Cu) (tedit 5D9F72B1)
    (at 77.875001 62.700001)
    (descr "SOIC, 16 Pin (JEDEC MS-012AC, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U3 (at 0.065 6.35) (layer B.SilkS))
    (fp_text value CH340G (at 0 -5.9) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -2.475 4.445) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 7 Board_1-GND))
    (pad 2 smd roundrect (at -2.475 3.175) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 23 "Board_1-Net-(R9-Pad2)"))
    (pad 3 smd roundrect (at -2.475 1.905) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 22 "Board_1-Net-(R8-Pad2)"))
    (pad 4 smd roundrect (at -2.475 0.635) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 Board_1-+3V3))
    (pad 5 smd roundrect (at -2.475 -0.635) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 Board_1-D+))
    (pad 6 smd roundrect (at -2.475 -1.905) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 5 Board_1-D-))
    (pad 7 smd roundrect (at -2.475 -3.175) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 11 "Board_1-Net-(C3-Pad1)"))
    (pad 8 smd roundrect (at -2.475 -4.445) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 12 "Board_1-Net-(C5-Pad1)"))
    (pad 9 smd roundrect (at 2.475 -4.445) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 28 "Board_1-Net-(U3-Pad9)"))
    (pad 10 smd roundrect (at 2.475 -3.175) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 24 "Board_1-Net-(U3-Pad10)"))
    (pad 11 smd roundrect (at 2.475 -1.905) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 25 "Board_1-Net-(U3-Pad11)"))
    (pad 12 smd roundrect (at 2.475 -0.635) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 26 "Board_1-Net-(U3-Pad12)"))
    (pad 13 smd roundrect (at 2.475 0.635) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 6 Board_1-DTR))
    (pad 14 smd roundrect (at 2.475 1.905) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 30 Board_1-RTS))
    (pad 15 smd roundrect (at 2.475 3.175) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 27 "Board_1-Net-(U3-Pad15)"))
    (pad 16 smd roundrect (at 2.475 4.445) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 Board_1-+3V3))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-16_3.9x9.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystal:Crystal_HC49-4H_Vertical (layer B.Cu) (tedit 5A1AD3B7)
    (at 68.850001 62.700001 180)
    (descr "Crystal THT HC-49-4H http://5hertz.com/pdfs/04404_D.pdf")
    (tags "THT crystalHC-49-4H")
    (fp_text reference Y1 (at 1.07 3.525) (layer B.SilkS))
    (fp_text value Crystal (at 2.44 -3.525) (layer B.Fab))
    (fp_text user %R (at 2.44 0) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Board_1-Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 4.88 0 180) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Board_1-Net-(C5-Pad1)"))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_HC49-4H_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D10.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 54.445001 55.715001)
    (descr "LED, diameter 10.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LED10-4500RT%23KIN.pdf")
    (tags "LED diameter 10.0mm 2 pins")
    (fp_text reference D1 (at 1.27 -1.905) (layer F.SilkS))
    (fp_text value LED (at 1.27 6.56) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 13 "Board_1-Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 Board_1-+5V))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D10.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D10.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 54.445001 67.145001)
    (descr "LED, diameter 10.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LED10-4500RT%23KIN.pdf")
    (tags "LED diameter 10.0mm 2 pins")
    (fp_text reference D2 (at 1.27 -1.905) (layer F.SilkS))
    (fp_text value LED (at 1.27 6.56) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 13 "Board_1-Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 Board_1-+5V))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D10.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D10.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 70.955001 55.715001)
    (descr "LED, diameter 10.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LED10-4500RT%23KIN.pdf")
    (tags "LED diameter 10.0mm 2 pins")
    (fp_text reference D3 (at 1.27 -1.905) (layer F.SilkS))
    (fp_text value LED (at 1.27 6.56) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 14 "Board_1-Net-(D3-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 Board_1-+5V))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D10.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D10.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 82.385001 55.715001)
    (descr "LED, diameter 10.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LED10-4500RT%23KIN.pdf")
    (tags "LED diameter 10.0mm 2 pins")
    (fp_text reference D4 (at 1.27 -1.905) (layer F.SilkS))
    (fp_text value LED (at 1.27 6.56) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 14 "Board_1-Net-(D3-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 Board_1-+5V))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D10.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D10.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 98.895001 55.715001)
    (descr "LED, diameter 10.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LED10-4500RT%23KIN.pdf")
    (tags "LED diameter 10.0mm 2 pins")
    (fp_text reference D5 (at 1.27 -1.905) (layer F.SilkS))
    (fp_text value LED (at 1.27 6.56) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 15 "Board_1-Net-(D5-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 Board_1-+5V))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D10.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D10.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 98.895001 67.145001)
    (descr "LED, diameter 10.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LED10-4500RT%23KIN.pdf")
    (tags "LED diameter 10.0mm 2 pins")
    (fp_text reference D6 (at 1.27 -1.905) (layer F.SilkS))
    (fp_text value LED (at 1.27 6.56) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 15 "Board_1-Net-(D5-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 Board_1-+5V))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D10.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module semaforBoard:PinHeader_1x02_P2.54mm_Vertical (layer B.Cu) (tedit 5EE4CC18)
    (at 98.895001 69.685001 270)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J1 (at 0 2.33 90) (layer B.SilkS))
    (fp_text value RESET (at 0 -4.87 90) (layer B.Fab))
    (fp_text user %R (at 0 -1.27 180) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 Board_1-RESET))
    (pad 2 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 Board_1-GND))
  )
  (gr_line (start 82.2621 100.719) (end 73.6179 100.719) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 82.3594 100.7142) (end 82.2621 100.719) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 82.4555 100.7) (end 82.3594 100.7142) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 82.5497 100.6764) (end 82.4555 100.7) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 82.6412 100.6436) (end 82.5497 100.6764) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 82.729 100.6021) (end 82.6412 100.6436) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 82.8123 100.5522) (end 82.729 100.6021) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 82.8904 100.4943) (end 82.8123 100.5522) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 82.9624 100.429) (end 82.8904 100.4943) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 83.0276 100.3571) (end 82.9624 100.429) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 83.0855 100.279) (end 83.0276 100.3571) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 83.1354 100.1957) (end 83.0855 100.279) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 83.177 100.1079) (end 83.1354 100.1957) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 83.2097 100.0164) (end 83.177 100.1079) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 83.2333 99.9221) (end 83.2097 100.0164) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 83.2476 99.826) (end 83.2333 99.9221) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 83.2523 99.7288) (end 83.2476 99.826) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 83.2523 99.2112) (end 83.2523 99.7288) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 83.2476 99.1139) (end 83.2523 99.2112) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 83.2333 99.0178) (end 83.2476 99.1139) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 83.2097 98.9236) (end 83.2333 99.0178) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 83.177 98.8321) (end 83.2097 98.9236) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 83.1354 98.7443) (end 83.177 98.8321) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 83.0855 98.661) (end 83.1354 98.7443) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 83.0276 98.5829) (end 83.0855 98.661) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 82.9624 98.5109) (end 83.0276 98.5829) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 82.8904 98.4457) (end 82.9624 98.5109) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 82.8123 98.3878) (end 82.8904 98.4457) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 82.729 98.3379) (end 82.8123 98.3878) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 82.6412 98.2963) (end 82.729 98.3379) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 82.5497 98.2636) (end 82.6412 98.2963) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 82.4555 98.24) (end 82.5497 98.2636) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 82.3594 98.2257) (end 82.4555 98.24) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 82.2621 98.221) (end 82.3594 98.2257) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.6179 98.2209) (end 82.2621 98.221) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.5206 98.2257) (end 73.6179 98.2209) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.4245 98.24) (end 73.5206 98.2257) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.3303 98.2636) (end 73.4245 98.24) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.2388 98.2963) (end 73.3303 98.2636) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.151 98.3378) (end 73.2388 98.2963) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.0677 98.3878) (end 73.151 98.3378) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.9896 98.4457) (end 73.0677 98.3878) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.9176 98.5109) (end 72.9896 98.4457) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.8524 98.5829) (end 72.9176 98.5109) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.7945 98.6609) (end 72.8524 98.5829) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.7446 98.7443) (end 72.7945 98.6609) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.703 98.8321) (end 72.7446 98.7443) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.6703 98.9236) (end 72.703 98.8321) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.6467 99.0178) (end 72.6703 98.9236) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.6324 99.1139) (end 72.6467 99.0178) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.6277 99.2112) (end 72.6324 99.1139) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.6277 99.7288) (end 72.6277 99.2112) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.6324 99.826) (end 72.6277 99.7288) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.6467 99.9221) (end 72.6324 99.826) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.6703 100.0164) (end 72.6467 99.9221) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.703 100.1079) (end 72.6703 100.0164) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.7446 100.1957) (end 72.703 100.1079) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.7945 100.279) (end 72.7446 100.1957) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.8524 100.357) (end 72.7945 100.279) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.9176 100.429) (end 72.8524 100.357) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.9896 100.4943) (end 72.9176 100.429) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.0677 100.5522) (end 72.9896 100.4943) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.151 100.6021) (end 73.0677 100.5522) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.2388 100.6436) (end 73.151 100.6021) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.3303 100.6764) (end 73.2388 100.6436) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.4245 100.7) (end 73.3303 100.6764) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.5206 100.7142) (end 73.4245 100.7) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.6179 100.719) (end 73.5206 100.7142) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 82.2621 126.079) (end 73.6179 126.079) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 82.3594 126.0742) (end 82.2621 126.079) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 82.4555 126.06) (end 82.3594 126.0742) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 82.5497 126.0364) (end 82.4555 126.06) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 82.6412 126.0036) (end 82.5497 126.0364) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 82.729 125.9621) (end 82.6412 126.0036) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 82.8123 125.9122) (end 82.729 125.9621) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 82.8904 125.8543) (end 82.8123 125.9122) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 82.9624 125.789) (end 82.8904 125.8543) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 83.0276 125.7171) (end 82.9624 125.789) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 83.0855 125.639) (end 83.0276 125.7171) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 83.1354 125.5557) (end 83.0855 125.639) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 83.177 125.4679) (end 83.1354 125.5557) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 83.2097 125.3764) (end 83.177 125.4679) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 83.2333 125.2822) (end 83.2097 125.3764) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 83.2476 125.1861) (end 83.2333 125.2822) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 83.2523 125.0888) (end 83.2476 125.1861) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 83.2523 124.5712) (end 83.2523 125.0888) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 83.2476 124.4739) (end 83.2523 124.5712) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 83.2333 124.3778) (end 83.2476 124.4739) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 83.2097 124.2836) (end 83.2333 124.3778) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 83.177 124.1921) (end 83.2097 124.2836) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 83.1354 124.1043) (end 83.177 124.1921) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 83.0855 124.021) (end 83.1354 124.1043) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 83.0276 123.9429) (end 83.0855 124.021) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 82.9624 123.8709) (end 83.0276 123.9429) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 82.8904 123.8057) (end 82.9624 123.8709) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 82.8123 123.7478) (end 82.8904 123.8057) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 82.729 123.6979) (end 82.8123 123.7478) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 82.6412 123.6563) (end 82.729 123.6979) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 82.5497 123.6236) (end 82.6412 123.6563) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 82.4555 123.6) (end 82.5497 123.6236) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 82.3594 123.5857) (end 82.4555 123.6) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 82.2621 123.581) (end 82.3594 123.5857) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.6179 123.5809) (end 82.2621 123.581) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.5206 123.5857) (end 73.6179 123.5809) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.4245 123.6) (end 73.5206 123.5857) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.3303 123.6236) (end 73.4245 123.6) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.2388 123.6563) (end 73.3303 123.6236) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.151 123.6979) (end 73.2388 123.6563) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.0677 123.7478) (end 73.151 123.6979) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.9896 123.8057) (end 73.0677 123.7478) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.9176 123.8709) (end 72.9896 123.8057) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.8524 123.9429) (end 72.9176 123.8709) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.7945 124.0209) (end 72.8524 123.9429) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.7446 124.1043) (end 72.7945 124.0209) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.703 124.1921) (end 72.7446 124.1043) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.6703 124.2836) (end 72.703 124.1921) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.6467 124.3778) (end 72.6703 124.2836) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.6324 124.4739) (end 72.6467 124.3778) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.6277 124.5712) (end 72.6324 124.4739) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.6277 125.0888) (end 72.6277 124.5712) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.6324 125.186) (end 72.6277 125.0888) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.6467 125.2821) (end 72.6324 125.186) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.6703 125.3764) (end 72.6467 125.2821) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.703 125.4679) (end 72.6703 125.3764) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.7446 125.5557) (end 72.703 125.4679) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.7945 125.639) (end 72.7446 125.5557) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.8524 125.7171) (end 72.7945 125.639) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.9176 125.789) (end 72.8524 125.7171) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.9896 125.8543) (end 72.9176 125.789) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.0677 125.9122) (end 72.9896 125.8543) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.151 125.9621) (end 73.0677 125.9122) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.2388 126.0036) (end 73.151 125.9621) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.3303 126.0364) (end 73.2388 126.0036) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.4245 126.06) (end 73.3303 126.0364) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.5206 126.0742) (end 73.4245 126.06) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.6179 126.079) (end 73.5206 126.0742) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.6277 74.3688) (end 72.6277 73.8512) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.6324 74.466) (end 72.6277 74.3688) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.6467 74.5621) (end 72.6324 74.466) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.6703 74.6564) (end 72.6467 74.5621) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.703 74.7479) (end 72.6703 74.6564) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.7446 74.8357) (end 72.703 74.7479) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.7945 74.919) (end 72.7446 74.8357) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.8524 74.997) (end 72.7945 74.919) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.9176 75.069) (end 72.8524 74.997) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.9896 75.1343) (end 72.9176 75.069) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.0677 75.1921) (end 72.9896 75.1343) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.151 75.2421) (end 73.0677 75.1921) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.2388 75.2836) (end 73.151 75.2421) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.3303 75.3164) (end 73.2388 75.2836) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.4245 75.34) (end 73.3303 75.3164) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.5206 75.3542) (end 73.4245 75.34) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.6179 75.359) (end 73.5206 75.3542) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 82.2621 75.359) (end 73.6179 75.359) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 82.3594 75.3542) (end 82.2621 75.359) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 82.4555 75.34) (end 82.3594 75.3542) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 82.5497 75.3164) (end 82.4555 75.34) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 82.6412 75.2836) (end 82.5497 75.3164) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 82.729 75.2421) (end 82.6412 75.2836) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 82.8123 75.1922) (end 82.729 75.2421) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 82.8904 75.1343) (end 82.8123 75.1922) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 82.9624 75.069) (end 82.8904 75.1343) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 83.0276 74.997) (end 82.9624 75.069) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 83.0855 74.919) (end 83.0276 74.997) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 83.1354 74.8357) (end 83.0855 74.919) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 83.177 74.7479) (end 83.1354 74.8357) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 83.2097 74.6564) (end 83.177 74.7479) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 83.2333 74.5621) (end 83.2097 74.6564) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 83.2476 74.466) (end 83.2333 74.5621) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 83.2523 74.3688) (end 83.2476 74.466) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 83.2523 73.8512) (end 83.2523 74.3688) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 83.2476 73.7539) (end 83.2523 73.8512) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 83.2333 73.6578) (end 83.2476 73.7539) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 83.2097 73.5636) (end 83.2333 73.6578) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 83.177 73.4721) (end 83.2097 73.5636) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 83.1354 73.3843) (end 83.177 73.4721) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 83.0855 73.3009) (end 83.1354 73.3843) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 83.0276 73.2229) (end 83.0855 73.3009) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 82.9624 73.1509) (end 83.0276 73.2229) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 82.8904 73.0857) (end 82.9624 73.1509) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 82.8123 73.0278) (end 82.8904 73.0857) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 82.729 72.9779) (end 82.8123 73.0278) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 82.6412 72.9363) (end 82.729 72.9779) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 82.5497 72.9036) (end 82.6412 72.9363) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 82.4555 72.88) (end 82.5497 72.9036) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 82.3594 72.8657) (end 82.4555 72.88) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 82.2621 72.861) (end 82.3594 72.8657) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.6179 72.8609) (end 82.2621 72.861) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.5206 72.8657) (end 73.6179 72.8609) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.4245 72.88) (end 73.5206 72.8657) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.3303 72.9036) (end 73.4245 72.88) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.2388 72.9363) (end 73.3303 72.9036) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.151 72.9778) (end 73.2388 72.9363) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.0677 73.0278) (end 73.151 72.9778) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.9896 73.0857) (end 73.0677 73.0278) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.9176 73.1509) (end 72.9896 73.0857) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.8524 73.2229) (end 72.9176 73.1509) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.7945 73.3009) (end 72.8524 73.2229) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.7446 73.3843) (end 72.7945 73.3009) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.703 73.4721) (end 72.7446 73.3843) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.6703 73.5636) (end 72.703 73.4721) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.6467 73.6578) (end 72.6703 73.5636) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.6324 73.7539) (end 72.6467 73.6578) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.6277 73.8512) (end 72.6324 73.7539) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 100.1652 75.3591) (end 92.2446 75.359) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 100.7622 75.3906) (end 100.1652 75.3591) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 101.3404 75.4819) (end 100.7622 75.3906) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 101.3661 75.4873) (end 101.3404 75.4819) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 101.9315 75.6392) (end 101.3661 75.4873) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 102.4776 75.8485) (end 101.9315 75.6392) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 102.5016 75.8591) (end 102.4776 75.8485) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 103.0226 76.125) (end 102.5016 75.8591) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 103.5137 76.4435) (end 103.0226 76.125) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 103.535 76.4589) (end 103.5137 76.4435) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 103.9893 76.8273) (end 103.535 76.4589) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 104.4128 77.2507) (end 103.9893 76.8273) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 104.7811 77.705) (end 104.4128 77.2507) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 104.7965 77.7263) (end 104.7811 77.705) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.1148 78.217) (end 104.7965 77.7263) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.3808 78.7384) (end 105.1148 78.217) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.3915 78.7624) (end 105.3808 78.7384) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.6008 79.3086) (end 105.3915 78.7624) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.7527 79.8739) (end 105.6008 79.3086) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.7581 79.8993) (end 105.7527 79.8739) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.8494 80.4778) (end 105.7581 79.8993) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.881 81.0814) (end 105.8494 80.4778) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.881 92.4985) (end 105.881 81.0814) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.8504 93.0893) (end 105.881 92.4985) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.8476 93.1155) (end 105.8504 93.0893) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.7558 93.6931) (end 105.8476 93.1155) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.6046 94.2586) (end 105.7558 93.6931) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.5965 94.2836) (end 105.6046 94.2586) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.3866 94.8296) (end 105.5965 94.2836) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.1212 95.3513) (end 105.3866 94.8296) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.108 95.374) (end 105.1212 95.3513) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 104.7889 95.8648) (end 105.108 95.374) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 104.4127 96.3294) (end 104.7889 95.8648) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 103.9991 96.7435) (end 104.4127 96.3294) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 103.9795 96.7611) (end 103.9991 96.7435) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 103.535 97.1211) (end 103.9795 96.7611) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 103.5138 97.1365) (end 103.535 97.1211) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 103.0226 97.4551) (end 103.5138 97.1365) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 102.49 97.7264) (end 103.0226 97.4551) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 101.9315 97.9408) (end 102.49 97.7264) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 101.3659 98.0928) (end 101.9315 97.9408) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 101.3404 98.0982) (end 101.3659 98.0928) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 100.7627 98.1893) (end 101.3404 98.0982) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 100.1649 98.2209) (end 100.7627 98.1893) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 92.2446 98.221) (end 100.1649 98.2209) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 92.1473 98.2258) (end 92.2446 98.221) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 92.0512 98.24) (end 92.1473 98.2258) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.957 98.2636) (end 92.0512 98.24) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.8655 98.2964) (end 91.957 98.2636) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.7777 98.3379) (end 91.8655 98.2964) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.6943 98.3878) (end 91.7777 98.3379) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.6163 98.4457) (end 91.6943 98.3878) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.5443 98.511) (end 91.6163 98.4457) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.4791 98.5829) (end 91.5443 98.511) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.4212 98.661) (end 91.4791 98.5829) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.3712 98.7443) (end 91.4212 98.661) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.3297 98.8321) (end 91.3712 98.7443) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.297 98.9236) (end 91.3297 98.8321) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.2734 99.0178) (end 91.297 98.9236) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.2591 99.1139) (end 91.2734 99.0178) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.2543 99.2112) (end 91.2591 99.1139) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.2543 99.7288) (end 91.2543 99.2112) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.2591 99.8261) (end 91.2543 99.7288) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.2734 99.9222) (end 91.2591 99.8261) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.297 100.0164) (end 91.2734 99.9222) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.3297 100.1079) (end 91.297 100.0164) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.3712 100.1957) (end 91.3297 100.1079) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.4212 100.279) (end 91.3712 100.1957) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.4791 100.3571) (end 91.4212 100.279) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.5443 100.429) (end 91.4791 100.3571) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.6163 100.4943) (end 91.5443 100.429) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.6943 100.5522) (end 91.6163 100.4943) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.7777 100.6021) (end 91.6943 100.5522) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.8655 100.6436) (end 91.7777 100.6021) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.957 100.6764) (end 91.8655 100.6436) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 92.0512 100.7) (end 91.957 100.6764) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 92.1473 100.7142) (end 92.0512 100.7) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 92.2446 100.719) (end 92.1473 100.7142) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 100.1652 100.7191) (end 92.2446 100.719) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 100.7622 100.7507) (end 100.1652 100.7191) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 101.3404 100.8419) (end 100.7622 100.7507) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 101.3661 100.8473) (end 101.3404 100.8419) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 101.9186 100.9954) (end 101.3661 100.8473) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 101.9436 101.0035) (end 101.9186 100.9954) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 102.49 101.2136) (end 101.9436 101.0035) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 103.0113 101.4788) (end 102.49 101.2136) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 103.034 101.492) (end 103.0113 101.4788) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 103.5137 101.8035) (end 103.034 101.492) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 103.535 101.8189) (end 103.5137 101.8035) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 103.9893 102.1873) (end 103.535 101.8189) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 104.4035 102.601) (end 103.9893 102.1873) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 104.4211 102.6205) (end 104.4035 102.601) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 104.7889 103.0753) (end 104.4211 102.6205) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.1148 103.577) (end 104.7889 103.0753) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.3866 104.1105) (end 105.1148 103.577) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.5965 104.6564) (end 105.3866 104.1105) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.6046 104.6811) (end 105.5965 104.6564) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.7557 105.2464) (end 105.6046 104.6811) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.8476 105.8245) (end 105.7557 105.2464) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.8504 105.8507) (end 105.8476 105.8245) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.8809 106.4351) (end 105.8504 105.8507) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.8807 117.8716) (end 105.8809 106.4351) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.8494 118.4622) (end 105.8807 117.8716) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.7582 119.0404) (end 105.8494 118.4622) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.7527 119.0661) (end 105.7582 119.0404) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.6008 119.6315) (end 105.7527 119.0661) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.3866 120.1896) (end 105.6008 119.6315) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.1212 120.7113) (end 105.3866 120.1896) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.108 120.734) (end 105.1212 120.7113) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 104.7892 121.2244) (end 105.108 120.734) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 104.4127 121.6894) (end 104.7892 121.2244) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 103.9991 122.1035) (end 104.4127 121.6894) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 103.9795 122.1211) (end 103.9991 122.1035) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 103.535 122.4811) (end 103.9795 122.1211) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 103.5138 122.4965) (end 103.535 122.4811) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 103.0226 122.8151) (end 103.5138 122.4965) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 102.49 123.0864) (end 103.0226 122.8151) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 101.9315 123.3009) (end 102.49 123.0864) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 101.3659 123.4528) (end 101.9315 123.3009) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 101.3404 123.4582) (end 101.3659 123.4528) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 100.7627 123.5493) (end 101.3404 123.4582) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 100.1649 123.5809) (end 100.7627 123.5493) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 92.2446 123.581) (end 100.1649 123.5809) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 92.1473 123.5858) (end 92.2446 123.581) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 92.0512 123.6) (end 92.1473 123.5858) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.957 123.6236) (end 92.0512 123.6) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.8655 123.6564) (end 91.957 123.6236) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.7777 123.6979) (end 91.8655 123.6564) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.6943 123.7478) (end 91.7777 123.6979) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.6163 123.8057) (end 91.6943 123.7478) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.5443 123.871) (end 91.6163 123.8057) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.4791 123.9429) (end 91.5443 123.871) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.4212 124.021) (end 91.4791 123.9429) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.3712 124.1043) (end 91.4212 124.021) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.3297 124.1921) (end 91.3712 124.1043) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.297 124.2836) (end 91.3297 124.1921) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.2734 124.3778) (end 91.297 124.2836) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.2591 124.4739) (end 91.2734 124.3778) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.2543 124.5712) (end 91.2591 124.4739) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.2543 125.0888) (end 91.2543 124.5712) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.2591 125.1861) (end 91.2543 125.0888) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.2734 125.2822) (end 91.2591 125.1861) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.297 125.3764) (end 91.2734 125.2822) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.3297 125.4679) (end 91.297 125.3764) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.3712 125.5557) (end 91.3297 125.4679) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.4212 125.639) (end 91.3712 125.5557) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.4791 125.7171) (end 91.4212 125.639) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.5443 125.789) (end 91.4791 125.7171) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.6163 125.8543) (end 91.5443 125.789) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.6943 125.9122) (end 91.6163 125.8543) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.7777 125.9621) (end 91.6943 125.9122) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.8655 126.0037) (end 91.7777 125.9621) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.957 126.0364) (end 91.8655 126.0037) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 92.0512 126.06) (end 91.957 126.0364) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 92.1473 126.0742) (end 92.0512 126.06) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 92.2446 126.079) (end 92.1473 126.0742) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 100.1652 126.0791) (end 92.2446 126.079) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 100.7622 126.1107) (end 100.1652 126.0791) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 101.3404 126.2019) (end 100.7622 126.1107) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 101.3661 126.2073) (end 101.3404 126.2019) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 101.931 126.359) (end 101.3661 126.2073) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 102.4896 126.5734) (end 101.931 126.359) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 103.0113 126.8388) (end 102.4896 126.5734) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 103.034 126.852) (end 103.0113 126.8388) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 103.5137 127.1635) (end 103.034 126.852) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 103.535 127.179) (end 103.5137 127.1635) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 103.9897 127.5477) (end 103.535 127.179) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 104.4124 127.9703) (end 103.9897 127.5477) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 104.7889 128.4353) (end 104.4124 127.9703) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.108 128.926) (end 104.7889 128.4353) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.1212 128.9487) (end 105.108 128.926) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.3864 129.47) (end 105.1212 128.9487) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.5965 130.0164) (end 105.3864 129.47) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.6046 130.0414) (end 105.5965 130.0164) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.7557 130.6064) (end 105.6046 130.0414) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.8476 131.1845) (end 105.7557 130.6064) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.8504 131.2107) (end 105.8476 131.1845) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.881 131.8015) (end 105.8504 131.2107) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.881 143.2185) (end 105.881 131.8015) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.8504 143.8094) (end 105.881 143.2185) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.8476 143.8355) (end 105.8504 143.8094) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.7558 144.4131) (end 105.8476 143.8355) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.601 144.991) (end 105.7558 144.4131) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.3866 145.5496) (end 105.601 144.991) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.1211 146.0715) (end 105.3866 145.5496) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.108 146.0941) (end 105.1211 146.0715) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 104.7889 146.5848) (end 105.108 146.0941) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 104.4211 147.0395) (end 104.7889 146.5848) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 104.4035 147.0591) (end 104.4211 147.0395) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 103.9897 147.4724) (end 104.4035 147.0591) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 103.535 147.8411) (end 103.9897 147.4724) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 103.5138 147.8565) (end 103.535 147.8411) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 103.023 148.1748) (end 103.5138 147.8565) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 102.4895 148.4467) (end 103.023 148.1748) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 101.9436 148.6565) (end 102.4895 148.4467) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 101.9186 148.6647) (end 101.9436 148.6565) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 101.3536 148.8157) (end 101.9186 148.6647) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 100.7755 148.9077) (end 101.3536 148.8157) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 100.7494 148.9104) (end 100.7755 148.9077) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 100.1715 148.9407) (end 100.7494 148.9104) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 55.7151 148.9408) (end 100.1715 148.9407) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 55.1173 148.9092) (end 55.7151 148.9408) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 54.5396 148.8181) (end 55.1173 148.9092) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 54.5139 148.8126) (end 54.5396 148.8181) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 53.949 148.6609) (end 54.5139 148.8126) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 53.4024 148.4515) (end 53.949 148.6609) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 53.3784 148.4408) (end 53.4024 148.4515) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 52.8685 148.181) (end 53.3784 148.4408) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 52.846 148.168) (end 52.8685 148.181) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 52.3556 147.8491) (end 52.846 148.168) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.8907 147.4727) (end 52.3556 147.8491) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.4673 147.0493) (end 51.8907 147.4727) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.099 146.595) (end 51.4673 147.0493) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.0835 146.5737) (end 51.099 146.595) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.772 146.094) (end 51.0835 146.5737) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.7589 146.0713) (end 50.772 146.094) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.4936 145.55) (end 50.7589 146.0713) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.2835 145.0036) (end 50.4936 145.55) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.2754 144.9786) (end 50.2835 145.0036) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.1243 144.4136) (end 50.2754 144.9786) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.0307 143.8227) (end 50.1243 144.4136) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.999 143.2185) (end 50.0307 143.8227) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.9991 131.7949) (end 49.999 143.2185) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.0307 131.1973) (end 49.9991 131.7949) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.1243 130.6064) (end 50.0307 131.1973) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.2792 130.0285) (end 50.1243 130.6064) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.4885 129.4824) (end 50.2792 130.0285) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.4991 129.4584) (end 50.4885 129.4824) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.7652 128.937) (end 50.4991 129.4584) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.0911 128.4352) (end 50.7652 128.937) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.4676 127.9703) (end 51.0911 128.4352) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.8907 127.5473) (end 51.4676 127.9703) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 52.3552 127.1711) (end 51.8907 127.5473) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 52.857 126.8452) (end 52.3552 127.1711) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 53.39 126.5736) (end 52.857 126.8452) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 53.9485 126.3592) (end 53.39 126.5736) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 54.5139 126.2073) (end 53.9485 126.3592) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 54.5396 126.2019) (end 54.5139 126.2073) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 55.1178 126.1107) (end 54.5396 126.2019) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 55.7149 126.0791) (end 55.1178 126.1107) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 63.6354 126.079) (end 55.7149 126.0791) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 63.7327 126.0742) (end 63.6354 126.079) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 63.8288 126.06) (end 63.7327 126.0742) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 63.923 126.0364) (end 63.8288 126.06) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.0145 126.0036) (end 63.923 126.0364) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.1023 125.9621) (end 64.0145 126.0036) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.1857 125.9122) (end 64.1023 125.9621) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.2637 125.8543) (end 64.1857 125.9122) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.3357 125.789) (end 64.2637 125.8543) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.4009 125.717) (end 64.3357 125.789) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.4588 125.639) (end 64.4009 125.717) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.5088 125.5557) (end 64.4588 125.639) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.5503 125.4679) (end 64.5088 125.5557) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.583 125.3764) (end 64.5503 125.4679) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.6066 125.2821) (end 64.583 125.3764) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.6209 125.186) (end 64.6066 125.2821) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.6257 125.0888) (end 64.6209 125.186) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.6257 124.5712) (end 64.6257 125.0888) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.6209 124.4739) (end 64.6257 124.5712) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.6066 124.3778) (end 64.6209 124.4739) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.583 124.2835) (end 64.6066 124.3778) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.5503 124.1921) (end 64.583 124.2835) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.5088 124.1043) (end 64.5503 124.1921) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.4588 124.0209) (end 64.5088 124.1043) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.4009 123.9429) (end 64.4588 124.0209) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.3357 123.8709) (end 64.4009 123.9429) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.2637 123.8057) (end 64.3357 123.8709) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.1857 123.7478) (end 64.2637 123.8057) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.1023 123.6978) (end 64.1857 123.7478) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.0145 123.6563) (end 64.1023 123.6978) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 63.923 123.6236) (end 64.0145 123.6563) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 63.8288 123.6) (end 63.923 123.6236) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 63.7327 123.5857) (end 63.8288 123.6) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 63.6354 123.5809) (end 63.7327 123.5857) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 55.7151 123.5808) (end 63.6354 123.5809) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 55.1173 123.5492) (end 55.7151 123.5808) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 54.5396 123.4581) (end 55.1173 123.5492) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 54.5142 123.4527) (end 54.5396 123.4581) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 53.9485 123.3007) (end 54.5142 123.4527) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 53.3905 123.0865) (end 53.9485 123.3007) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 52.8574 122.8149) (end 53.3905 123.0865) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 52.3663 122.4965) (end 52.8574 122.8149) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 52.345 122.481) (end 52.3663 122.4965) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.9005 122.121) (end 52.345 122.481) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.881 122.1035) (end 51.9005 122.121) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.4673 121.6893) (end 51.881 122.1035) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.0911 121.2247) (end 51.4673 121.6893) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.772 120.734) (end 51.0911 121.2247) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.7589 120.7113) (end 50.772 120.734) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.4936 120.19) (end 50.7589 120.7113) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.2835 119.6436) (end 50.4936 120.19) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.2754 119.6186) (end 50.2835 119.6436) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.1243 119.0536) (end 50.2754 119.6186) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.0324 118.4755) (end 50.1243 119.0536) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.0296 118.4494) (end 50.0324 118.4755) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.999 117.8585) (end 50.0296 118.4494) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.999 106.4414) (end 49.999 117.8585) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.0307 105.8373) (end 49.999 106.4414) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.1218 105.2596) (end 50.0307 105.8373) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.1272 105.2342) (end 50.1218 105.2596) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.2792 104.6685) (end 50.1272 105.2342) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.4885 104.1224) (end 50.2792 104.6685) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.4991 104.0984) (end 50.4885 104.1224) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.7588 103.5888) (end 50.4991 104.0984) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.772 103.566) (end 50.7588 103.5888) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.0908 103.0756) (end 50.772 103.566) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.4589 102.6205) (end 51.0908 103.0756) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.4765 102.601) (end 51.4589 102.6205) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.8903 102.1876) (end 51.4765 102.601) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 52.3552 101.8111) (end 51.8903 102.1876) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 52.857 101.4852) (end 52.3552 101.8111) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 53.3905 101.2134) (end 52.857 101.4852) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 53.9485 100.9992) (end 53.3905 101.2134) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 54.5264 100.8443) (end 53.9485 100.9992) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 55.1173 100.7507) (end 54.5264 100.8443) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 55.7084 100.7193) (end 55.1173 100.7507) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 63.6354 100.719) (end 55.7084 100.7193) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 63.7327 100.7142) (end 63.6354 100.719) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 63.8288 100.7) (end 63.7327 100.7142) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 63.923 100.6764) (end 63.8288 100.7) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.0145 100.6436) (end 63.923 100.6764) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.1023 100.6021) (end 64.0145 100.6436) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.1857 100.5521) (end 64.1023 100.6021) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.2637 100.4943) (end 64.1857 100.5521) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.3357 100.429) (end 64.2637 100.4943) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.4009 100.357) (end 64.3357 100.429) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.4588 100.279) (end 64.4009 100.357) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.5088 100.1957) (end 64.4588 100.279) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.5503 100.1079) (end 64.5088 100.1957) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.583 100.0164) (end 64.5503 100.1079) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.6066 99.9221) (end 64.583 100.0164) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.6209 99.826) (end 64.6066 99.9221) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.6257 99.7288) (end 64.6209 99.826) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.6257 99.2112) (end 64.6257 99.7288) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.6209 99.1139) (end 64.6257 99.2112) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.6066 99.0178) (end 64.6209 99.1139) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.583 98.9235) (end 64.6066 99.0178) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.5503 98.8321) (end 64.583 98.9235) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.5088 98.7442) (end 64.5503 98.8321) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.4588 98.6609) (end 64.5088 98.7442) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.4009 98.5829) (end 64.4588 98.6609) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.3357 98.5109) (end 64.4009 98.5829) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.2637 98.4456) (end 64.3357 98.5109) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.1857 98.3878) (end 64.2637 98.4456) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.1023 98.3378) (end 64.1857 98.3878) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.0145 98.2963) (end 64.1023 98.3378) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 63.923 98.2636) (end 64.0145 98.2963) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 63.8288 98.24) (end 63.923 98.2636) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 63.7327 98.2257) (end 63.8288 98.24) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 63.6354 98.2209) (end 63.7327 98.2257) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 55.7151 98.2208) (end 63.6354 98.2209) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 55.1173 98.1892) (end 55.7151 98.2208) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 54.5396 98.0981) (end 55.1173 98.1892) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 54.5142 98.0927) (end 54.5396 98.0981) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 53.949 97.9409) (end 54.5142 98.0927) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 53.4024 97.7315) (end 53.949 97.9409) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 53.3784 97.7208) (end 53.4024 97.7315) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 52.8688 97.4611) (end 53.3784 97.7208) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 52.846 97.448) (end 52.8688 97.4611) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 52.3552 97.1288) (end 52.846 97.448) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.8907 96.7527) (end 52.3552 97.1288) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.4676 96.3296) (end 51.8907 96.7527) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.0988 95.8748) (end 51.4676 96.3296) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.0835 95.8537) (end 51.0988 95.8748) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.765 95.3625) (end 51.0835 95.8537) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.4992 94.8416) (end 50.765 95.3625) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.4885 94.8176) (end 50.4992 94.8416) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.2792 94.2714) (end 50.4885 94.8176) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.1273 93.7061) (end 50.2792 94.2714) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.1219 93.6804) (end 50.1273 93.7061) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.0324 93.1155) (end 50.1219 93.6804) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.0297 93.0896) (end 50.0324 93.1155) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.999 92.4985) (end 50.0297 93.0896) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.999 81.0816) (end 49.999 92.4985) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.0296 80.4907) (end 49.999 81.0816) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.0324 80.4645) (end 50.0296 80.4907) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.1218 79.8996) (end 50.0324 80.4645) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.1273 79.8739) (end 50.1218 79.8996) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.279 79.309) (end 50.1273 79.8739) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.4885 78.7624) (end 50.279 79.309) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.4991 78.7384) (end 50.4885 78.7624) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.765 78.2174) (end 50.4991 78.7384) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.0911 77.7152) (end 50.765 78.2174) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.4589 77.2605) (end 51.0911 77.7152) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.4765 77.241) (end 51.4589 77.2605) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.8903 76.8276) (end 51.4765 77.241) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 52.345 76.459) (end 51.8903 76.8276) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 52.3662 76.4435) (end 52.345 76.459) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 52.857 76.1252) (end 52.3662 76.4435) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 53.39 75.8536) (end 52.857 76.1252) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 53.9485 75.6392) (end 53.39 75.8536) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 54.5264 75.4843) (end 53.9485 75.6392) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 55.1173 75.3907) (end 54.5264 75.4843) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 55.7084 75.3593) (end 55.1173 75.3907) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 63.6354 75.359) (end 55.7084 75.3593) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 63.7327 75.3542) (end 63.6354 75.359) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 63.8288 75.34) (end 63.7327 75.3542) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 63.923 75.3164) (end 63.8288 75.34) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.0145 75.2836) (end 63.923 75.3164) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.1023 75.2421) (end 64.0145 75.2836) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.1857 75.1921) (end 64.1023 75.2421) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.2637 75.1343) (end 64.1857 75.1921) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.3357 75.069) (end 64.2637 75.1343) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.4009 74.997) (end 64.3357 75.069) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.4588 74.919) (end 64.4009 74.997) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.5088 74.8357) (end 64.4588 74.919) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.5503 74.7479) (end 64.5088 74.8357) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.583 74.6564) (end 64.5503 74.7479) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.6066 74.5621) (end 64.583 74.6564) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.6209 74.466) (end 64.6066 74.5621) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.6257 74.3688) (end 64.6209 74.466) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.6257 73.8512) (end 64.6257 74.3688) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.6209 73.7539) (end 64.6257 73.8512) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.6066 73.6578) (end 64.6209 73.7539) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.583 73.5635) (end 64.6066 73.6578) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.5503 73.4721) (end 64.583 73.5635) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.5088 73.3842) (end 64.5503 73.4721) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.4588 73.3009) (end 64.5088 73.3842) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.4009 73.2229) (end 64.4588 73.3009) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.3357 73.1509) (end 64.4009 73.2229) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.2637 73.0856) (end 64.3357 73.1509) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.1857 73.0278) (end 64.2637 73.0856) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.1023 72.9778) (end 64.1857 73.0278) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.0145 72.9363) (end 64.1023 72.9778) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 63.923 72.9036) (end 64.0145 72.9363) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 63.8288 72.8799) (end 63.923 72.9036) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 63.7327 72.8657) (end 63.8288 72.8799) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 63.6354 72.8609) (end 63.7327 72.8657) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 55.7151 72.8608) (end 63.6354 72.8609) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 55.1173 72.8292) (end 55.7151 72.8608) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 54.5396 72.738) (end 55.1173 72.8292) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 54.5142 72.7327) (end 54.5396 72.738) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 53.9485 72.5807) (end 54.5142 72.7327) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 53.3905 72.3665) (end 53.9485 72.5807) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 52.8574 72.0949) (end 53.3905 72.3665) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 52.3663 71.7764) (end 52.8574 72.0949) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 52.345 71.761) (end 52.3663 71.7764) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.9005 71.401) (end 52.345 71.761) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.881 71.3835) (end 51.9005 71.401) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.4673 70.9692) (end 51.881 71.3835) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.099 70.515) (end 51.4673 70.9692) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.0835 70.4937) (end 51.099 70.515) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.7653 70.003) (end 51.0835 70.4937) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.4992 69.4816) (end 50.7653 70.003) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.4885 69.4576) (end 50.4992 69.4816) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.279 68.9109) (end 50.4885 69.4576) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.1273 68.3461) (end 50.279 68.9109) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.1219 68.3204) (end 50.1273 68.3461) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.0306 67.7422) (end 50.1219 68.3204) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.9991 67.1449) (end 50.0306 67.7422) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.999 55.7216) (end 49.9991 67.1449) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.0296 55.1307) (end 49.999 55.7216) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.0324 55.1045) (end 50.0296 55.1307) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.1242 54.5269) (end 50.0324 55.1045) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.279 53.949) (end 50.1242 54.5269) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.4934 53.3905) (end 50.279 53.949) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.7589 52.8685) (end 50.4934 53.3905) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.772 52.846) (end 50.7589 52.8685) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.0911 52.3552) (end 50.772 52.846) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.4589 51.9005) (end 51.0911 52.3552) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.4765 51.881) (end 51.4589 51.9005) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.8903 51.4676) (end 51.4765 51.881) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 52.345 51.0989) (end 51.8903 51.4676) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 52.3662 51.0835) (end 52.345 51.0989) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 52.857 50.7652) (end 52.3662 51.0835) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 53.3905 50.4934) (end 52.857 50.7652) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 53.9364 50.2835) (end 53.3905 50.4934) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 53.9614 50.2754) (end 53.9364 50.2835) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 54.5264 50.1243) (end 53.9614 50.2754) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 55.1045 50.0324) (end 54.5264 50.1243) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 55.1306 50.0296) (end 55.1045 50.0324) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 55.7085 49.9993) (end 55.1306 50.0296) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 100.1649 49.9991) (end 55.7085 49.9993) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 100.7627 50.0307) (end 100.1649 49.9991) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 101.3404 50.1218) (end 100.7627 50.0307) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 101.3661 50.1273) (end 101.3404 50.1218) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 101.931 50.279) (end 101.3661 50.1273) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 102.4776 50.4885) (end 101.931 50.279) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 102.5016 50.4991) (end 102.4776 50.4885) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 103.0115 50.7589) (end 102.5016 50.4991) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 103.034 50.772) (end 103.0115 50.7589) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 103.5244 51.0908) (end 103.034 50.772) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 103.9893 51.4673) (end 103.5244 51.0908) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 104.4128 51.8907) (end 103.9893 51.4673) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 104.7811 52.345) (end 104.4128 51.8907) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 104.7965 52.3662) (end 104.7811 52.345) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.108 52.846) (end 104.7965 52.3662) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.1212 52.8687) (end 105.108 52.846) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.3864 53.39) (end 105.1212 52.8687) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.5965 53.9364) (end 105.3864 53.39) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.6046 53.9614) (end 105.5965 53.9364) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.7557 54.5264) (end 105.6046 53.9614) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.8493 55.1173) (end 105.7557 54.5264) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.881 55.7215) (end 105.8493 55.1173) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.8809 67.1452) (end 105.881 55.7215) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.8493 67.7427) (end 105.8809 67.1452) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.7557 68.3336) (end 105.8493 67.7427) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.601 68.911) (end 105.7557 68.3336) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.3866 69.4696) (end 105.601 68.911) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.115 70.0026) (end 105.3866 69.4696) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 104.7889 70.5048) (end 105.115 70.0026) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 104.4124 70.9697) (end 104.7889 70.5048) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 103.9991 71.3835) (end 104.4124 70.9697) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 103.9795 71.4011) (end 103.9991 71.3835) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 103.5243 71.7692) (end 103.9795 71.4011) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 103.034 72.088) (end 103.5243 71.7692) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 103.0113 72.1012) (end 103.034 72.088) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 102.5016 72.3608) (end 103.0113 72.1012) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 102.4776 72.3715) (end 102.5016 72.3608) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 101.9315 72.5808) (end 102.4776 72.3715) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 101.3661 72.7327) (end 101.9315 72.5808) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 101.3404 72.7382) (end 101.3661 72.7327) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 100.7627 72.8293) (end 101.3404 72.7382) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 100.1649 72.8609) (end 100.7627 72.8293) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 92.2446 72.861) (end 100.1649 72.8609) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 92.1473 72.8658) (end 92.2446 72.861) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 92.0512 72.88) (end 92.1473 72.8658) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.957 72.9036) (end 92.0512 72.88) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.8655 72.9364) (end 91.957 72.9036) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.7777 72.9779) (end 91.8655 72.9364) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.6943 73.0278) (end 91.7777 72.9779) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.6163 73.0857) (end 91.6943 73.0278) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.5443 73.151) (end 91.6163 73.0857) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.4791 73.2229) (end 91.5443 73.151) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.4212 73.301) (end 91.4791 73.2229) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.3712 73.3843) (end 91.4212 73.301) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.3297 73.4721) (end 91.3712 73.3843) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.297 73.5636) (end 91.3297 73.4721) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.2734 73.6578) (end 91.297 73.5636) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.2591 73.7539) (end 91.2734 73.6578) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.2543 73.8512) (end 91.2591 73.7539) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.2543 74.3688) (end 91.2543 73.8512) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.2591 74.466) (end 91.2543 74.3688) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.2734 74.5621) (end 91.2591 74.466) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.297 74.6564) (end 91.2734 74.5621) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.3297 74.7479) (end 91.297 74.6564) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.3712 74.8357) (end 91.3297 74.7479) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.4212 74.919) (end 91.3712 74.8357) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.4791 74.997) (end 91.4212 74.919) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.5443 75.069) (end 91.4791 74.997) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.6163 75.1343) (end 91.5443 75.069) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.6943 75.1922) (end 91.6163 75.1343) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.7777 75.2421) (end 91.6943 75.1922) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.8655 75.2836) (end 91.7777 75.2421) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.957 75.3164) (end 91.8655 75.2836) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 92.0512 75.34) (end 91.957 75.3164) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 92.1473 75.3542) (end 92.0512 75.34) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 92.2446 75.359) (end 92.1473 75.3542) (layer Edge.Cuts) (width 0.1))
  (gr_text "06/20\nSemafor v0.2" (at 92.545001 127.350028 90) (layer F.SilkS))
  (gr_text reset (at 96.863001 147.670028) (layer B.SilkS))
  (gr_text "06/20\nSemafor v0.2" (at 92.545001 101.990019 90) (layer F.SilkS))
  (gr_text reset (at 96.863001 122.310019) (layer B.SilkS))
  (gr_text "06/20\nSemafor v0.2" (at 92.545001 76.63001 90) (layer F.SilkS))
  (gr_text reset (at 96.863001 96.95001) (layer B.SilkS))
  (gr_text "06/20\nSemafor v0.2" (at 92.545001 51.270001 90) (layer F.SilkS))
  (gr_text reset (at 96.863001 71.590001) (layer B.SilkS))
)
